(kicad_pcb (version 4) (host pcbnew no-vcs-found-product)
  (general
    (links 30)
    (no_connects 0)
    (area 126.586499 101.1333 197.210262 127.3397)
    (thickness 1.6)
    (drawings 13)
    (tracks 53)
    (zones 0)
    (modules 19)
    (nets 33)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.2032)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.127)
    (pcb_text_size 1.27 1.27)
    (mod_edge_width 0.15)
    (mod_text_size 1.016 1.016)
    (mod_text_width 0.127)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x310fc_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.127000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerbers/))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 GND)
  (net 3 off_audio)
  (net 4 "Net-(C2-Pad2)")
  (net 5 "Net-(D1-Pad2)")
  (net 6 "Net-(J1-Pad3)")
  (net 7 "Net-(J1-Pad2)")
  (net 8 +5V)
  (net 9 tx328)
  (net 10 "Net-(R1-Pad2)")
  (net 11 "Net-(R4-Pad2)")
  (net 12 "Net-(U1-Pad1)")
  (net 13 rx328)
  (net 14 "Net-(U1-Pad6)")
  (net 15 "Net-(U2-Pad24)")
  (net 16 "Net-(U2-Pad25)")
  (net 17 "Net-(U2-Pad27)")
  (net 18 "Net-(U2-Pad28)")
  (net 19 "Net-(U2-Pad29)")
  (net 20 "Net-(U2-Pad23)")
  (net 21 "Net-(U2-Pad21)")
  (net 22 "Net-(U2-Pad10)")
  (net 23 "Net-(U2-Pad8)")
  (net 24 "Net-(U2-Pad6)")
  (net 25 "Net-(U2-Pad7)")
  (net 26 "Net-(U2-Pad5)")
  (net 27 "Net-(U2-Pad4)")
  (net 28 "Net-(U2-Pad3)")
  (net 29 "Net-(U2-Pad1)")
  (net 30 Vin)
  (net 31 "Net-(U2-Pad2)")
  (net 32 bias_vol)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R4-Pad2)")
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U2-Pad1)")
    (add_net "Net-(U2-Pad10)")
    (add_net "Net-(U2-Pad2)")
    (add_net "Net-(U2-Pad21)")
    (add_net "Net-(U2-Pad23)")
    (add_net "Net-(U2-Pad24)")
    (add_net "Net-(U2-Pad25)")
    (add_net "Net-(U2-Pad27)")
    (add_net "Net-(U2-Pad28)")
    (add_net "Net-(U2-Pad29)")
    (add_net "Net-(U2-Pad3)")
    (add_net "Net-(U2-Pad4)")
    (add_net "Net-(U2-Pad5)")
    (add_net "Net-(U2-Pad6)")
    (add_net "Net-(U2-Pad7)")
    (add_net "Net-(U2-Pad8)")
    (add_net Vin)
    (add_net bias_vol)
    (add_net off_audio)
    (add_net rx328)
    (add_net tx328)
  )
  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer F.Cu) (tedit 55AD888B)
    (at 151.765 120.65 90)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C1 (at 1.27 2.54 270) (layer F.SilkS))
    (fp_text value 220nF (at 1.27 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer F.Cu) (tedit 55AD8892)
    (at 151.765 109.22 90)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C2 (at 1.27 2.54 270) (layer F.SilkS))
    (fp_text value 220nF (at 1.27 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 3 off_audio))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(C2-Pad2)"))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer F.Cu) (tedit 55ADC0A5)
    (at 161.29 112.395 270)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C3 (at 1.27 2.286 450) (layer F.SilkS))
    (fp_text value 1uF (at 1.27 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 32 bias_vol))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:STX-3120-3B (layer F.Cu) (tedit 55AAF497)
    (at 133.35 114.3)
    (fp_text reference J1 (at 2.54 2.54) (layer F.SilkS))
    (fp_text value TRS (at -3.81 -1.27) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.9 1.9) (drill 1.35) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole circle (at 5 5) (size 1.9 1.9) (drill 1.35) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(J1-Pad3)"))
    (pad 2 thru_hole circle (at 5 -5) (size 1.9 1.9) (drill 1.35) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(J1-Pad2)"))
    (pad "" np_thru_hole circle (at 0 5) (size 1.65 1.65) (drill 1.65) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 0 -5) (size 1.65 1.65) (drill 1.65) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 5 0) (size 1.65 1.65) (drill 1.65) (layers *.Cu *.Mask F.SilkS))
  )
  (module DonB:1pin (layer F.Cu) (tedit 55AD8FE4)
    (at 175.26 118.11)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference P1 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value GND (at 0 -2.159) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 2.286 2.286) (drill 1.5113) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND) (clearance 0.254))
  )
  (module DonB:1pin (layer F.Cu) (tedit 55AD8FC8)
    (at 175.26 109.22)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference P2 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value Vin (at 0 2.54) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 2.286 2.286) (drill 1.5113) (layers *.Cu *.Mask F.SilkS)
      (net 30 Vin) (clearance 0.254))
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 55AB0D52)
    (at 185.42 113.665 90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R1 (at 0 0 90) (layer F.SilkS))
    (fp_text value 1K (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -5.08 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 9 tx328))
    (pad 2 thru_hole circle (at 5.08 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 10 "Net-(R1-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 55AB0D56)
    (at 180.34 113.665 270)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R2 (at 0 0 270) (layer F.SilkS))
    (fp_text value 2K (at 0 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at -5.08 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 10 "Net-(R1-Pad2)"))
    (pad 2 thru_hole circle (at 5.08 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 2 GND))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 55AB1478)
    (at 148.59 113.665 270)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R3 (at 0 0 270) (layer F.SilkS))
    (fp_text value 220R (at 0 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at -5.08 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 4 "Net-(C2-Pad2)"))
    (pad 2 thru_hole circle (at 5.08 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 55AB08F4)
    (at 165.1 113.665 90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R5 (at 0 0 90) (layer F.SilkS))
    (fp_text value 680R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -5.08 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 32 bias_vol))
    (pad 2 thru_hole circle (at 5.08 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 3 off_audio))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 55AB08F9)
    (at 170.18 113.665 90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R6 (at 0 0 90) (layer F.SilkS))
    (fp_text value 47K (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -5.08 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 32 bias_vol))
    (pad 2 thru_hole circle (at 5.08 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 8 +5V))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 55AB08FD)
    (at 167.64 113.665 270)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R7 (at 0 0 270) (layer F.SilkS))
    (fp_text value 47K (at 0 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at -5.08 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 5.08 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 32 bias_vol))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:OS102011 (layer F.Cu) (tedit 55AAF49F)
    (at 144.78 114.3 270)
    (fp_text reference SW1 (at 0 -4 270) (layer F.SilkS) hide)
    (fp_text value Switch_SPDT_x2 (at 0 3.75 270) (layer F.SilkS) hide)
    (pad 2 thru_hole circle (at 0 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(C1-Pad1)"))
    (pad 3 thru_hole circle (at 2 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(J1-Pad3)"))
    (pad 1 thru_hole circle (at -2 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(J1-Pad2)"))
    (pad 4 thru_hole circle (at -4.1 0 270) (size 2 2) (drill 1.5) (layers *.Cu *.Mask F.SilkS))
    (pad 5 thru_hole circle (at 4.1 0 270) (size 2 2) (drill 1.5) (layers *.Cu *.Mask F.SilkS))
  )
  (module DonB:Molex-22-15-2066 (layer F.Cu) (tedit 55A998B3)
    (at 194.31 113.665)
    (fp_text reference U1 (at 0 12.7) (layer F.SilkS))
    (fp_text value HC-05 (at 0 -11.43) (layer F.Fab))
    (pad 1 thru_hole circle (at -5.334 -6.35) (size 1.524 1.524) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(U1-Pad1)"))
    (pad 2 thru_hole circle (at -5.334 -3.81) (size 1.524 1.524) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(R1-Pad2)"))
    (pad 3 thru_hole circle (at -5.334 -1.27) (size 1.524 1.524) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 13 rx328))
    (pad 4 thru_hole circle (at -5.334 1.27) (size 1.524 1.524) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 5 thru_hole circle (at -5.334 3.81) (size 1.524 1.524) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 8 +5V))
    (pad 6 thru_hole circle (at -5.334 6.35) (size 1.524 1.524) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(U1-Pad6)"))
  )
  (module LEDs:LED-0805 (layer F.Cu) (tedit 55AD8B8B)
    (at 138.43 106.68)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D1 (at 2.54 -0.635) (layer F.SilkS))
    (fp_text value RX (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 180) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 180) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module DonB:R_0805_HandSoldering (layer F.Cu) (tedit 55AD8B89)
    (at 144.145 106.68)
    (descr "Resistor, SMD, 0805, Hand soldering,")
    (tags "Resistor, SMD, 0805, Hand soldering,")
    (attr smd)
    (fp_text reference R4 (at 3.175 -0.635) (layer F.SilkS))
    (fp_text value 220R (at -0.3175 0.109999) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.30048 0) (size 1.50114 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D1-Pad2)"))
    (pad 2 smd rect (at 1.30048 0) (size 1.50114 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(R4-Pad2)"))
    (model smd/resistors/R0805/R0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:Arduino_Mini_Pro_Skel (layer B.Cu) (tedit 55AF1757)
    (at 171.45 113.665 90)
    (fp_text reference U2 (at 0 8.89 90) (layer B.SilkS))
    (fp_text value ArduinoMiniPro (at 0 -2.54 180) (layer B.SilkS))
    (pad 24 thru_hole circle (at 7.62 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 15 "Net-(U2-Pad24)"))
    (pad 25 thru_hole circle (at 7.62 -2.54 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 16 "Net-(U2-Pad25)"))
    (pad 26 thru_hole circle (at 7.62 -5.08 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 3 off_audio))
    (pad 27 thru_hole circle (at 7.62 -7.62 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 17 "Net-(U2-Pad27)"))
    (pad 28 thru_hole circle (at 7.62 -10.16 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 18 "Net-(U2-Pad28)"))
    (pad 29 thru_hole circle (at 7.62 -12.7 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 19 "Net-(U2-Pad29)"))
    (pad 30 thru_hole circle (at 7.62 -15.24 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 11 "Net-(R4-Pad2)"))
    (pad 23 thru_hole circle (at 7.62 2.54 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 20 "Net-(U2-Pad23)"))
    (pad 22 thru_hole circle (at 7.62 5.08 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 8 +5V))
    (pad 21 thru_hole circle (at 7.62 7.62 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 21 "Net-(U2-Pad21)"))
    (pad 20 thru_hole circle (at 7.62 10.16 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 2 GND))
    (pad 19 thru_hole circle (at 7.62 12.7 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 30 Vin))
    (pad 12 thru_hole circle (at -7.62 12.7 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 9 tx328))
    (pad 11 thru_hole circle (at -7.62 10.16 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 13 rx328))
    (pad 10 thru_hole circle (at -7.62 7.62 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 22 "Net-(U2-Pad10)"))
    (pad 9 thru_hole circle (at -7.62 5.08 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 2 GND))
    (pad 8 thru_hole circle (at -7.62 2.54 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 23 "Net-(U2-Pad8)"))
    (pad 6 thru_hole circle (at -7.62 -2.54 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 24 "Net-(U2-Pad6)"))
    (pad 7 thru_hole circle (at -7.62 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 25 "Net-(U2-Pad7)"))
    (pad 5 thru_hole circle (at -7.62 -5.08 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 26 "Net-(U2-Pad5)"))
    (pad 4 thru_hole circle (at -7.62 -7.62 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 27 "Net-(U2-Pad4)"))
    (pad 3 thru_hole circle (at -7.62 -10.16 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 28 "Net-(U2-Pad3)"))
    (pad 2 thru_hole circle (at -7.62 -12.7 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 31 "Net-(U2-Pad2)"))
    (pad 1 thru_hole circle (at -7.62 -15.24 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 29 "Net-(U2-Pad1)"))
  )
  (module DonB:1pin (layer F.Cu) (tedit 55ADB5CF)
    (at 157.48 118.11)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference P3 (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value TP1 (at 0 -2.032) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 2.286 2.286) (drill 1.5113) (layers *.Cu *.Mask F.SilkS)
      (net 32 bias_vol) (clearance 0.254))
  )
  (module DonB:1pin (layer F.Cu) (tedit 55ADB5CB)
    (at 157.48 109.22 90)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference P4 (at -0.3175 0.109999 180) (layer F.SilkS) hide)
    (fp_text value TP2 (at -2.286 0 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.286 2.286) (drill 1.5113) (layers *.Cu *.Mask F.SilkS)
      (net 3 off_audio) (clearance 0.254))
  )
  (gr_text "K\n" (at 136.271 106.68) (layer F.SilkS))
  (gr_text "Don Bindner" (at 140.97 114.046 90) (layer B.SilkS))
  (gr_text "APRS Companion" (at 135.763 113.792 90) (layer B.SilkS))
  (gr_text L (at 142.875 108.585) (layer F.SilkS))
  (gr_text R (at 142.875 120.015) (layer F.SilkS))
  (gr_text Vcc (at 191.77 117.475) (layer B.SilkS))
  (gr_text GND (at 191.77 114.935) (layer B.SilkS))
  (gr_text TX (at 191.77 112.395) (layer B.SilkS))
  (gr_text RX (at 191.77 109.855) (layer B.SilkS))
  (gr_line (start 131.445 104.775) (end 131.445 122.555) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 194.31 104.775) (end 131.445 104.775) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 194.31 122.555) (end 194.31 104.775) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 131.445 122.555) (end 194.31 122.555) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2032))
    (min_thickness 0.2032)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 193.929 122.174) (xy 131.826 122.174) (xy 131.826 105.156) (xy 193.929 105.156)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2032))
    (min_thickness 0.2032)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 193.929 122.174) (xy 131.826 122.174) (xy 131.826 105.156) (xy 193.929 105.156)
      )
    )
  )
)
