(kicad_pcb (version 4) (host pcbnew 0.201505262310+5684~23~ubuntu14.04.1-product)
  (general
    (links 6)
    (no_connects 0)
    (area 140.97 91.44 165.100001 116.840001)
    (thickness 1.6)
    (drawings 19)
    (tracks 22)
    (zones 0)
    (modules 12)
    (nets 7)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.4)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerbers/))
  )
  (net 0 "")
  (net 1 "Net-(P1-Pad1)")
  (net 2 "Net-(P2-Pad1)")
  (net 3 "Net-(P3-Pad1)")
  (net 4 "Net-(P4-Pad1)")
  (net 5 "Net-(P12-Pad1)")
  (net 6 "Net-(P10-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.4)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(P1-Pad1)")
    (add_net "Net-(P10-Pad1)")
    (add_net "Net-(P12-Pad1)")
    (add_net "Net-(P2-Pad1)")
    (add_net "Net-(P3-Pad1)")
    (add_net "Net-(P4-Pad1)")
  )
  (module DonB:TESTPIN (layer F.Cu) (tedit 556BDB42)
    (at 149.86 101.6)
    (fp_text reference P1 (at 0 -7.62) (layer F.SilkS) hide)
    (fp_text value Vcc (at 0 -3.175 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.651 1.651) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(P1-Pad1)"))
  )
  (module DonB:TESTPIN (layer F.Cu) (tedit 556BDB57)
    (at 149.86 104.14)
    (fp_text reference P2 (at 0 7.62) (layer F.SilkS) hide)
    (fp_text value MISO (at 0 3.81 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.651 1.651) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(P2-Pad1)"))
  )
  (module DonB:TESTPIN (layer F.Cu) (tedit 556BDB44)
    (at 152.4 101.6)
    (fp_text reference P3 (at 0 -7.62) (layer F.SilkS) hide)
    (fp_text value MOSI (at 0 -3.81 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.651 1.651) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(P3-Pad1)"))
  )
  (module DonB:TESTPIN (layer F.Cu) (tedit 556BDB83)
    (at 152.4 104.14)
    (fp_text reference P4 (at 0 7.62) (layer F.SilkS) hide)
    (fp_text value SCK (at 0 4.064 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.651 1.651) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(P4-Pad1)"))
  )
  (module DonB:TESTPIN (layer F.Cu) (tedit 556BDB47)
    (at 154.94 101.6)
    (fp_text reference P5 (at 0 -7.62) (layer F.SilkS) hide)
    (fp_text value GND (at 0 -3.175 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.651 1.651) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(P12-Pad1)"))
  )
  (module DonB:TESTPIN (layer F.Cu) (tedit 556BDB69)
    (at 154.94 104.14)
    (fp_text reference P6 (at 0 7.62) (layer F.SilkS) hide)
    (fp_text value RESET (at 0 4.445 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.651 1.651) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(P10-Pad1)"))
  )
  (module DonB:TESTPIN (layer F.Cu) (tedit 556BDD88)
    (at 144.78 104.14)
    (fp_text reference P7 (at -2.54 0) (layer F.SilkS) hide)
    (fp_text value MISO (at 1.778 -0.254 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.651 1.651) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(P2-Pad1)"))
  )
  (module DonB:TESTPIN (layer F.Cu) (tedit 556BDD81)
    (at 144.78 106.68)
    (fp_text reference P8 (at -2.54 0) (layer F.SilkS) hide)
    (fp_text value MOSI (at 1.778 0.254 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.651 1.651) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(P3-Pad1)"))
  )
  (module DonB:TESTPIN (layer F.Cu) (tedit 556BDC86)
    (at 160.02 106.68)
    (fp_text reference P9 (at 2.54 0) (layer F.SilkS) hide)
    (fp_text value SCK (at -1.778 -0.508 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.651 1.651) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(P4-Pad1)"))
  )
  (module DonB:TESTPIN (layer F.Cu) (tedit 556BDC92)
    (at 160.02 109.22)
    (fp_text reference P10 (at 2.54 0) (layer F.SilkS) hide)
    (fp_text value RESET (at -1.778 0.508 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.651 1.651) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(P10-Pad1)"))
  )
  (module DonB:TESTPIN (layer F.Cu) (tedit 556BDC82)
    (at 160.02 99.06)
    (fp_text reference P11 (at 2.54 0) (layer F.SilkS) hide)
    (fp_text value Vcc (at -1.778 -0.254 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.651 1.651) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(P1-Pad1)"))
  )
  (module DonB:TESTPIN (layer F.Cu) (tedit 556BDC80)
    (at 160.02 101.6)
    (fp_text reference P12 (at 2.54 0) (layer F.SilkS) hide)
    (fp_text value GND (at -1.778 0.254 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.651 1.651) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(P12-Pad1)"))
  )
  (gr_text "Don Bindner	" (at 152.4 109.22) (layer B.SilkS))
  (gr_line (start 161.29 110.49) (end 161.29 96.52) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 160.02 111.76) (end 161.29 110.49) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.05 111.76) (end 160.02 111.76) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 143.51 109.22) (end 146.05 111.76) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 143.51 101.6) (end 143.51 109.22) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 149.86 95.25) (end 143.51 101.6) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 160.02 95.25) (end 149.86 95.25) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 161.29 96.52) (end 160.02 95.25) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 5) (net_name "Net-(P12-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 165.1 116.84) (xy 140.97 116.84) (xy 140.97 91.44) (xy 165.1 91.44)
      )
    )
  )
  (zone (net 5) (net_name "Net-(P12-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 165.1 116.84) (xy 140.97 116.84) (xy 140.97 91.44) (xy 165.1 91.44)
      )
    )
  )
)
