(kicad_pcb (version 4) (host pcbnew 0.201507012246+5852~23~ubuntu14.04.1-product)
  (general
    (links 111)
    (no_connects 0)
    (area 67.229691 108.6583 149.402001 152.1047)
    (thickness 1.6)
    (drawings 32)
    (tracks 390)
    (zones 0)
    (modules 53)
    (nets 65)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.651 1.651)
    (pad_drill 1.016)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerbers/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +BATT)
  (net 3 "Net-(C2-Pad1)")
  (net 4 "Net-(C2-Pad2)")
  (net 5 "Net-(C3-Pad1)")
  (net 6 "Net-(C3-Pad2)")
  (net 7 +3.3VP)
  (net 8 +3V3)
  (net 9 "Net-(C8-Pad1)")
  (net 10 "Net-(C10-Pad2)")
  (net 11 "Net-(C11-Pad2)")
  (net 12 "Net-(C12-Pad2)")
  (net 13 af_out)
  (net 14 led_tx)
  (net 15 "Net-(D2-Pad1)")
  (net 16 led_rx)
  (net 17 "Net-(D3-Pad1)")
  (net 18 ptt)
  (net 19 sig_out_1)
  (net 20 sig_out_2)
  (net 21 sig_out_3)
  (net 22 sig_out_4)
  (net 23 mosi)
  (net 24 miso)
  (net 25 sck)
  (net 26 "Net-(IC1-Pad19)")
  (net 27 "Net-(IC1-Pad22)")
  (net 28 a1)
  (net 29 "Net-(IC1-Pad25)")
  (net 30 "Net-(IC1-Pad26)")
  (net 31 rst)
  (net 32 rx328)
  (net 33 tx328)
  (net 34 mic_out)
  (net 35 txRadio)
  (net 36 rxRadio)
  (net 37 powerSave)
  (net 38 sq)
  (net 39 "Net-(R1-Pad1)")
  (net 40 "Net-(R1-Pad2)")
  (net 41 "Net-(U1-Pad1)")
  (net 42 rxNav)
  (net 43 txNav)
  (net 44 "Net-(U1-Pad4)")
  (net 45 "Net-(U1-Pad11)")
  (net 46 "Net-(U1-Pad13)")
  (net 47 "Net-(U1-Pad14)")
  (net 48 "Net-(U1-Pad15)")
  (net 49 serialRadio)
  (net 50 serial328)
  (net 51 "Net-(U1-Pad24)")
  (net 52 "Net-(U3-Pad8)")
  (net 53 "Net-(U3-Pad7)")
  (net 54 "Net-(IC1-Pad12)")
  (net 55 "Net-(IC1-Pad27)")
  (net 56 "Net-(IC1-Pad28)")
  (net 57 "Net-(U1-Pad8)")
  (net 58 "Net-(U1-Pad10)")
  (net 59 "Net-(U1-Pad21)")
  (net 60 "Net-(U1-Pad9)")
  (net 61 "Net-(IC1-Pad32)")
  (net 62 "Net-(U1-Pad12)")
  (net 63 sig_in_off)
  (net 64 "Net-(C10-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net GND)
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C10-Pad2)")
    (add_net "Net-(C11-Pad2)")
    (add_net "Net-(C12-Pad2)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(IC1-Pad12)")
    (add_net "Net-(IC1-Pad19)")
    (add_net "Net-(IC1-Pad22)")
    (add_net "Net-(IC1-Pad25)")
    (add_net "Net-(IC1-Pad26)")
    (add_net "Net-(IC1-Pad27)")
    (add_net "Net-(IC1-Pad28)")
    (add_net "Net-(IC1-Pad32)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad10)")
    (add_net "Net-(U1-Pad11)")
    (add_net "Net-(U1-Pad12)")
    (add_net "Net-(U1-Pad13)")
    (add_net "Net-(U1-Pad14)")
    (add_net "Net-(U1-Pad15)")
    (add_net "Net-(U1-Pad21)")
    (add_net "Net-(U1-Pad24)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U1-Pad8)")
    (add_net "Net-(U1-Pad9)")
    (add_net "Net-(U3-Pad7)")
    (add_net "Net-(U3-Pad8)")
    (add_net a1)
    (add_net af_out)
    (add_net led_rx)
    (add_net led_tx)
    (add_net mic_out)
    (add_net miso)
    (add_net mosi)
    (add_net powerSave)
    (add_net ptt)
    (add_net rst)
    (add_net rx328)
    (add_net rxNav)
    (add_net rxRadio)
    (add_net sck)
    (add_net serial328)
    (add_net serialRadio)
    (add_net sig_in_off)
    (add_net sig_out_1)
    (add_net sig_out_2)
    (add_net sig_out_3)
    (add_net sig_out_4)
    (add_net sq)
    (add_net tx328)
    (add_net txNav)
    (add_net txRadio)
  )
  (net_class C3-Pad1 ""
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(C3-Pad1)")
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3.3VP)
    (add_net +BATT)
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 5569076E)
    (at 127.635 121.285 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C1 (at 0 -2.3 90) (layer F.SilkS) hide)
    (fp_text value 10uF (at 0 2.3 90) (layer F.SilkS))
    (pad 1 smd rect (at -2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 smd rect (at 2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 +BATT))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:C_0805_HandSoldering (layer F.Cu) (tedit 5568B480)
    (at 146.05 118.745 180)
    (descr "SMT capacitor, 0805")
    (fp_text reference C2 (at 0 -2 180) (layer F.SilkS) hide)
    (fp_text value 2.2nF (at 0 1.905 180) (layer F.SilkS))
    (pad 1 smd rect (at 1.15062 0 180) (size 1.4986 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at -1.15062 0 180) (size 1.4986 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C2-Pad2)"))
    (model smd/Capacitors/C0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:C_0805_HandSoldering (layer F.Cu) (tedit 5569DECC)
    (at 122.809 118.745 270)
    (descr "SMT capacitor, 0805")
    (fp_text reference C3 (at 0 -2 270) (layer F.SilkS) hide)
    (fp_text value 10nF (at 0 1.778 270) (layer F.SilkS))
    (pad 1 smd rect (at 1.15062 0 270) (size 1.4986 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C3-Pad1)") (zone_connect 2))
    (pad 2 smd rect (at -1.15062 0 270) (size 1.4986 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C3-Pad2)"))
    (model smd/Capacitors/C0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:C_0805_HandSoldering (layer F.Cu) (tedit 5569D461)
    (at 135.89 127 90)
    (descr "SMT capacitor, 0805")
    (fp_text reference C4 (at 0 -2 90) (layer F.SilkS) hide)
    (fp_text value 22uF/10V (at -6.35 0 90) (layer F.SilkS))
    (pad 1 smd rect (at 1.15062 0 90) (size 1.4986 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -1.15062 0 90) (size 1.4986 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 7 +3.3VP))
    (model smd/Capacitors/C0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:C_0805_HandSoldering (layer F.Cu) (tedit 5569D463)
    (at 139.7 127 90)
    (descr "SMT capacitor, 0805")
    (fp_text reference C5 (at 0 -2 90) (layer F.SilkS) hide)
    (fp_text value 22uF/10V (at -6.35 0 90) (layer F.SilkS))
    (pad 1 smd rect (at 1.15062 0 90) (size 1.4986 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -1.15062 0 90) (size 1.4986 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 7 +3.3VP))
    (model smd/Capacitors/C0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:C_0805_HandSoldering (layer B.Cu) (tedit 55688F0D)
    (at 85.09 119.888 180)
    (descr "SMT capacitor, 0805")
    (fp_text reference C7 (at 0 2 180) (layer B.SilkS) hide)
    (fp_text value 100nF (at 0 1.778 180) (layer B.SilkS))
    (pad 1 smd rect (at 1.15062 0 180) (size 1.4986 1.4986) (layers B.Cu B.Paste B.Mask)
      (net 8 +3V3))
    (pad 2 smd rect (at -1.15062 0 180) (size 1.4986 1.4986) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model smd/Capacitors/C0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:C_0805_HandSoldering (layer F.Cu) (tedit 5569DBF8)
    (at 81.915 133.35 90)
    (descr "SMT capacitor, 0805")
    (fp_text reference C8 (at 0 -2 90) (layer F.SilkS) hide)
    (fp_text value 100nF (at -0.635 1.651 90) (layer F.SilkS))
    (pad 1 smd rect (at 1.15062 0 90) (size 1.4986 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C8-Pad1)"))
    (pad 2 smd rect (at -1.15062 0 90) (size 1.4986 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model smd/Capacitors/C0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:C_0805_HandSoldering (layer F.Cu) (tedit 5569DB64)
    (at 70.485 146.685 90)
    (descr "SMT capacitor, 0805")
    (fp_text reference C9 (at 0 -2 90) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.651 90) (layer F.SilkS))
    (pad 1 smd rect (at 1.15062 0 90) (size 1.4986 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C10-Pad2)"))
    (pad 2 smd rect (at -1.15062 0 90) (size 1.4986 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model smd/Capacitors/C0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:C_0805_HandSoldering (layer F.Cu) (tedit 5590CB47)
    (at 78.105 146.685 270)
    (descr "SMT capacitor, 0805")
    (fp_text reference C10 (at 4.445 0 270) (layer F.SilkS) hide)
    (fp_text value 1uF (at 0 -1.905 270) (layer F.SilkS))
    (pad 1 smd rect (at 1.15062 0 270) (size 1.4986 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(C10-Pad1)"))
    (pad 2 smd rect (at -1.15062 0 270) (size 1.4986 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C10-Pad2)"))
    (model smd/Capacitors/C0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:C_0805_HandSoldering (layer F.Cu) (tedit 5569DC4A)
    (at 85.09 116.84)
    (descr "SMT capacitor, 0805")
    (fp_text reference C11 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value 33pF (at -4.064 0) (layer F.SilkS))
    (pad 1 smd rect (at 1.15062 0) (size 1.4986 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -1.15062 0) (size 1.4986 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C11-Pad2)"))
    (model smd/Capacitors/C0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:C_0805_HandSoldering (layer F.Cu) (tedit 5569DC4D)
    (at 76.835 116.84 180)
    (descr "SMT capacitor, 0805")
    (fp_text reference C12 (at 0 -2 180) (layer F.SilkS) hide)
    (fp_text value 33pF (at 4.318 0 180) (layer F.SilkS))
    (pad 1 smd rect (at 1.15062 0 180) (size 1.4986 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -1.15062 0 180) (size 1.4986 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C12-Pad2)"))
    (model smd/Capacitors/C0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED-0805 (layer F.Cu) (tedit 55690540)
    (at 78.105 133.35 90)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D2 (at 0 -1.524 90) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.27 90) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 14 led_tx))
    (pad 1 smd rect (at -1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(D2-Pad1)"))
  )
  (module LEDs:LED-0805 (layer F.Cu) (tedit 556904EC)
    (at 70.485 133.35 90)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D3 (at 0 -1.524 90) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.27 90) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 16 led_rx))
    (pad 1 smd rect (at -1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(D3-Pad1)"))
  )
  (module Housings_QFP:TQFP-32_7x7mm_Pitch0.8mm (layer F.Cu) (tedit 556904DC)
    (at 80.899 124.206 270)
    (descr "32-Lead Plastic Thin Quad Flatpack (PT) - 7x7x1.0 mm Body, 2.00 mm [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.8")
    (attr smd)
    (fp_text reference IC1 (at -0.508 -1.016 270) (layer F.SilkS))
    (fp_text value ATMEGA328-A (at 0 6.05 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -4.25 -2.8 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 18 ptt))
    (pad 2 smd rect (at -4.25 -2 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 19 sig_out_1))
    (pad 3 smd rect (at -4.25 -1.2 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at -4.25 -0.4 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 8 +3V3))
    (pad 5 smd rect (at -4.25 0.4 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -4.25 1.2 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 8 +3V3))
    (pad 7 smd rect (at -4.25 2 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C11-Pad2)"))
    (pad 8 smd rect (at -4.25 2.8 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C12-Pad2)"))
    (pad 9 smd rect (at -2.8 4.25) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 20 sig_out_2))
    (pad 10 smd rect (at -2 4.25) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 21 sig_out_3))
    (pad 11 smd rect (at -1.2 4.25) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 22 sig_out_4))
    (pad 12 smd rect (at -0.4 4.25) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(IC1-Pad12)"))
    (pad 13 smd rect (at 0.4 4.25) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 16 led_rx))
    (pad 14 smd rect (at 1.2 4.25) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 14 led_tx))
    (pad 15 smd rect (at 2 4.25) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 23 mosi))
    (pad 16 smd rect (at 2.8 4.25) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 24 miso))
    (pad 17 smd rect (at 4.25 2.8 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 25 sck))
    (pad 18 smd rect (at 4.25 2 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 8 +3V3))
    (pad 19 smd rect (at 4.25 1.2 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(IC1-Pad19)"))
    (pad 20 smd rect (at 4.25 0.4 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C8-Pad1)"))
    (pad 21 smd rect (at 4.25 -0.4 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 22 smd rect (at 4.25 -1.2 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(IC1-Pad22)"))
    (pad 23 smd rect (at 4.25 -2 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 63 sig_in_off))
    (pad 24 smd rect (at 4.25 -2.8 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 28 a1))
    (pad 25 smd rect (at 2.8 -4.25) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(IC1-Pad25)"))
    (pad 26 smd rect (at 2 -4.25) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(IC1-Pad26)"))
    (pad 27 smd rect (at 1.2 -4.25) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(IC1-Pad27)"))
    (pad 28 smd rect (at 0.4 -4.25) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(IC1-Pad28)"))
    (pad 29 smd rect (at -0.4 -4.25) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 31 rst))
    (pad 30 smd rect (at -1.2 -4.25) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 32 rx328))
    (pad 31 smd rect (at -2 -4.25) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 33 tx328))
    (pad 32 smd rect (at -2.8 -4.25) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(IC1-Pad32)"))
    (model Housings_QFP.3dshapes/TQFP-32_7x7mm_Pitch0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:SRR1260 (layer F.Cu) (tedit 5569D8A5)
    (at 122.555 132.08 180)
    (fp_text reference L1 (at 0 -7.493 180) (layer F.SilkS))
    (fp_text value 12uH (at -3.81 -7.493 180) (layer F.SilkS))
    (pad 2 smd rect (at 6.1 0 180) (size 5.4 5.4) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C3-Pad1)") (zone_connect 2))
    (pad 1 smd rect (at -6.1 0 180) (size 5.4 5.4) (layers F.Cu F.Paste F.Mask)
      (net 7 +3.3VP) (zone_connect 2))
  )
  (module DonB:TESTPIN (layer F.Cu) (tedit 55690147)
    (at 111.76 147.32)
    (fp_text reference P1 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value mic_out (at 0 2) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.651 1.651) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 mic_out))
  )
  (module DonB:TESTPIN (layer F.Cu) (tedit 55690172)
    (at 111.76 144.78)
    (fp_text reference P2 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value txRadio (at 0 2) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.651 1.651) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 35 txRadio))
  )
  (module DonB:TESTPIN (layer F.Cu) (tedit 5569014F)
    (at 114.3 147.32)
    (fp_text reference P3 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value rxRadio (at 0 2) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.651 1.651) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 36 rxRadio))
  )
  (module DonB:TESTPIN (layer F.Cu) (tedit 55690154)
    (at 116.84 147.32)
    (fp_text reference P4 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value GND (at 0 2) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.651 1.651) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
  )
  (module DonB:TESTPIN (layer F.Cu) (tedit 5569016E)
    (at 114.3 144.78)
    (fp_text reference P5 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value GND (at 0 2) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.651 1.651) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
  )
  (module DonB:TESTPIN (layer F.Cu) (tedit 55690169)
    (at 116.84 144.78)
    (fp_text reference P6 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value +3.3V (at 0 2) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.651 1.651) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 +3.3VP))
  )
  (module DonB:TESTPIN (layer F.Cu) (tedit 55690157)
    (at 119.38 147.32)
    (fp_text reference P7 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value ptt (at 0 2) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.651 1.651) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 ptt))
  )
  (module DonB:TESTPIN (layer F.Cu) (tedit 55690160)
    (at 119.38 144.78)
    (fp_text reference P8 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value powerSave (at 0 2) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.651 1.651) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 37 powerSave))
  )
  (module DonB:TESTPIN (layer F.Cu) (tedit 5569015B)
    (at 121.92 147.32)
    (fp_text reference P9 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value sq (at 0 2) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.651 1.651) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 38 sq))
  )
  (module DonB:TESTPIN (layer F.Cu) (tedit 55690165)
    (at 121.92 144.78)
    (fp_text reference P10 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value af_out (at 0 2) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.651 1.651) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 af_out))
  )
  (module DonB:R_0805_HandSoldering (layer F.Cu) (tedit 540A4C46)
    (at 146.05 126.365 180)
    (descr "Resistor, SMD, 0805, Hand soldering,")
    (tags "Resistor, SMD, 0805, Hand soldering,")
    (attr smd)
    (fp_text reference R1 (at 0 -1.5 180) (layer F.SilkS) hide)
    (fp_text value 24K (at -0.08 1.524 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.30048 0 180) (size 1.50114 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(R1-Pad1)"))
    (pad 2 smd rect (at 1.30048 0 180) (size 1.50114 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(R1-Pad2)"))
    (model smd/resistors/R0805/R0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:R_0805_HandSoldering (layer F.Cu) (tedit 540A4C46)
    (at 146.05 122.555 180)
    (descr "Resistor, SMD, 0805, Hand soldering,")
    (tags "Resistor, SMD, 0805, Hand soldering,")
    (attr smd)
    (fp_text reference R2 (at 0 -1.5 180) (layer F.SilkS) hide)
    (fp_text value 10K (at -0.08 1.524 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.30048 0 180) (size 1.50114 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.30048 0 180) (size 1.50114 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(R1-Pad2)"))
    (model smd/resistors/R0805/R0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:R_0805_HandSoldering (layer F.Cu) (tedit 5568B47D)
    (at 146.05 114.935)
    (descr "Resistor, SMD, 0805, Hand soldering,")
    (tags "Resistor, SMD, 0805, Hand soldering,")
    (attr smd)
    (fp_text reference R3 (at 0 -1.5) (layer F.SilkS) hide)
    (fp_text value 8.2K (at 0 -1.905) (layer F.SilkS))
    (pad 1 smd rect (at -1.30048 0) (size 1.50114 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.30048 0) (size 1.50114 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C2-Pad2)"))
    (model smd/resistors/R0805/R0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:R_0805_HandSoldering (layer F.Cu) (tedit 540A4C46)
    (at 146.05 130.175 180)
    (descr "Resistor, SMD, 0805, Hand soldering,")
    (tags "Resistor, SMD, 0805, Hand soldering,")
    (attr smd)
    (fp_text reference R4 (at 0 -1.5 180) (layer F.SilkS) hide)
    (fp_text value 1.8K (at -0.08 1.524 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.30048 0 180) (size 1.50114 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(R1-Pad1)"))
    (pad 2 smd rect (at 1.30048 0 180) (size 1.50114 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 7 +3.3VP))
    (model smd/resistors/R0805/R0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:R_0805_HandSoldering (layer F.Cu) (tedit 5569DB94)
    (at 85.725 140.335 90)
    (descr "Resistor, SMD, 0805, Hand soldering,")
    (tags "Resistor, SMD, 0805, Hand soldering,")
    (attr smd)
    (fp_text reference R5 (at 0 -1.5 90) (layer F.SilkS) hide)
    (fp_text value 8.2K (at 1.651 1.905 90) (layer F.SilkS))
    (pad 1 smd rect (at -1.30048 0 90) (size 1.50114 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C10-Pad2)"))
    (pad 2 smd rect (at 1.30048 0 90) (size 1.50114 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 19 sig_out_1))
    (model smd/resistors/R0805/R0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:R_0805_HandSoldering (layer F.Cu) (tedit 5569DB7A)
    (at 74.295 140.335 90)
    (descr "Resistor, SMD, 0805, Hand soldering,")
    (tags "Resistor, SMD, 0805, Hand soldering,")
    (attr smd)
    (fp_text reference R6 (at 0 -1.5 90) (layer F.SilkS) hide)
    (fp_text value 3.9K (at -0.508 1.778 90) (layer F.SilkS))
    (pad 1 smd rect (at -1.30048 0 90) (size 1.50114 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C10-Pad2)"))
    (pad 2 smd rect (at 1.30048 0 90) (size 1.50114 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 20 sig_out_2))
    (model smd/resistors/R0805/R0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:R_0805_HandSoldering (layer F.Cu) (tedit 5569DB80)
    (at 78.105 140.335 90)
    (descr "Resistor, SMD, 0805, Hand soldering,")
    (tags "Resistor, SMD, 0805, Hand soldering,")
    (attr smd)
    (fp_text reference R7 (at 0 -1.5 90) (layer F.SilkS) hide)
    (fp_text value 2.2K (at -0.635 1.778 90) (layer F.SilkS))
    (pad 1 smd rect (at -1.30048 0 90) (size 1.50114 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C10-Pad2)"))
    (pad 2 smd rect (at 1.30048 0 90) (size 1.50114 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 21 sig_out_3))
    (model smd/resistors/R0805/R0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:R_0805_HandSoldering (layer F.Cu) (tedit 5569DB46)
    (at 81.915 140.335 90)
    (descr "Resistor, SMD, 0805, Hand soldering,")
    (tags "Resistor, SMD, 0805, Hand soldering,")
    (attr smd)
    (fp_text reference R8 (at 0 -1.5 90) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.651 90) (layer F.SilkS))
    (pad 1 smd rect (at -1.30048 0 90) (size 1.50114 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C10-Pad2)"))
    (pad 2 smd rect (at 1.30048 0 90) (size 1.50114 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 22 sig_out_4))
    (model smd/resistors/R0805/R0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:R_0805_HandSoldering (layer F.Cu) (tedit 558E3456)
    (at 74.295 146.685 270)
    (descr "Resistor, SMD, 0805, Hand soldering,")
    (tags "Resistor, SMD, 0805, Hand soldering,")
    (attr smd)
    (fp_text reference R9 (at 4.445 0 270) (layer F.SilkS) hide)
    (fp_text value 270R (at -0.381 -1.651 270) (layer F.SilkS))
    (pad 1 smd rect (at -1.30048 0 270) (size 1.50114 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C10-Pad2)"))
    (pad 2 smd rect (at 1.30048 0 270) (size 1.50114 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model smd/resistors/R0805/R0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:R_0805_HandSoldering (layer F.Cu) (tedit 5569DBD2)
    (at 74.295 133.35 270)
    (descr "Resistor, SMD, 0805, Hand soldering,")
    (tags "Resistor, SMD, 0805, Hand soldering,")
    (attr smd)
    (fp_text reference R10 (at 0 -1.5 270) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 -2.032 270) (layer F.SilkS))
    (pad 1 smd rect (at -1.30048 0 270) (size 1.50114 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.30048 0 270) (size 1.50114 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(D2-Pad1)"))
    (model smd/resistors/R0805/R0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:R_0805_HandSoldering (layer F.Cu) (tedit 5569DB87)
    (at 70.485 140.335 90)
    (descr "Resistor, SMD, 0805, Hand soldering,")
    (tags "Resistor, SMD, 0805, Hand soldering,")
    (attr smd)
    (fp_text reference R11 (at 0 -1.5 90) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.778 90) (layer F.SilkS))
    (pad 1 smd rect (at -1.30048 0 90) (size 1.50114 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.30048 0 90) (size 1.50114 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(D3-Pad1)"))
    (model smd/resistors/R0805/R0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:R_0805_HandSoldering (layer F.Cu) (tedit 5590CD0C)
    (at 81.915 146.685 270)
    (descr "Resistor, SMD, 0805, Hand soldering,")
    (tags "Resistor, SMD, 0805, Hand soldering,")
    (attr smd)
    (fp_text reference R12 (at 4.445 0 270) (layer F.SilkS) hide)
    (fp_text value 15K (at 0 -1.905 270) (layer F.SilkS))
    (pad 1 smd rect (at -1.30048 0 270) (size 1.50114 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(C10-Pad1)"))
    (pad 2 smd rect (at 1.30048 0 270) (size 1.50114 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 34 mic_out))
    (model smd/resistors/R0805/R0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:R_0805_HandSoldering (layer F.Cu) (tedit 5568A759)
    (at 103.505 113.03 90)
    (descr "Resistor, SMD, 0805, Hand soldering,")
    (tags "Resistor, SMD, 0805, Hand soldering,")
    (attr smd)
    (fp_text reference R16 (at 0 -1.5 90) (layer F.SilkS) hide)
    (fp_text value 1M (at 0 -1.524 90) (layer F.SilkS))
    (pad 1 smd rect (at -1.30048 0 90) (size 1.50114 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 28 a1))
    (pad 2 smd rect (at 1.30048 0 90) (size 1.50114 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 +BATT))
    (model smd/resistors/R0805/R0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:R_0805_HandSoldering (layer F.Cu) (tedit 540A4C46)
    (at 99.06 113.03 270)
    (descr "Resistor, SMD, 0805, Hand soldering,")
    (tags "Resistor, SMD, 0805, Hand soldering,")
    (attr smd)
    (fp_text reference R17 (at 0 -1.5 270) (layer F.SilkS) hide)
    (fp_text value 100K (at -0.08 1.524 270) (layer F.SilkS))
    (pad 1 smd rect (at -1.30048 0 270) (size 1.50114 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.30048 0 270) (size 1.50114 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 28 a1))
    (model smd/resistors/R0805/R0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-14_3.9x8.7mm_Pitch1.27mm (layer F.Cu) (tedit 5569DA6A)
    (at 99.06 124.46)
    (descr "14-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U4 (at 0 -5.375) (layer F.SilkS) hide)
    (fp_text value 4066 (at 0 -5.461) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 42 rxNav))
    (pad 2 smd rect (at -2.7 -2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 33 tx328))
    (pad 3 smd rect (at -2.7 -1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 32 rx328))
    (pad 4 smd rect (at -2.7 0) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 43 txNav))
    (pad 5 smd rect (at -2.7 1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 50 serial328))
    (pad 6 smd rect (at -2.7 2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 49 serialRadio))
    (pad 7 smd rect (at -2.7 3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 8 smd rect (at 2.7 3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 43 txNav))
    (pad 9 smd rect (at 2.7 2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 36 rxRadio))
    (pad 10 smd rect (at 2.7 1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 35 txRadio))
    (pad 11 smd rect (at 2.7 0) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 42 rxNav))
    (pad 12 smd rect (at 2.7 -1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 49 serialRadio))
    (pad 13 smd rect (at 2.7 -2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 50 serial328))
    (pad 14 smd rect (at 2.7 -3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 +3V3))
    (model Housings_SOIC.3dshapes/SOIC-14_3.9x8.7mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystals:Crystal_HC49-SD_SMD (layer F.Cu) (tedit 5569DC6D)
    (at 79.375 112.395 180)
    (descr "Crystal, Quarz, HC49-SD, SMD,")
    (tags "Crystal, Quarz, HC49-SD, SMD,")
    (attr smd)
    (fp_text reference Y1 (at 0 -0.254 180) (layer F.SilkS) hide)
    (fp_text value 8MHz (at 0 0 270) (layer F.SilkS))
    (pad 1 smd rect (at -4.84886 0 180) (size 5.6007 2.10058) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C11-Pad2)"))
    (pad 2 smd rect (at 4.84886 0 180) (size 5.6007 2.10058) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C12-Pad2)"))
  )
  (module DonB:Diode-SMB_Handsoldering (layer F.Cu) (tedit 55690463)
    (at 118.491 118.745 270)
    (descr "Diode SMB Handsoldering")
    (tags "Diode SMB Handsoldering")
    (attr smd)
    (fp_text reference D1 (at -4.572 2.54 270) (layer F.SilkS) hide)
    (fp_text value SSB43 (at 0 2.54 270) (layer F.SilkS))
    (fp_text user A (at -3.2004 1.95072 270) (layer F.SilkS))
    (fp_text user K (at 2.99974 1.95072 270) (layer F.SilkS))
    (pad 1 smd rect (at -2.70002 0 270) (size 3.50012 2.30124) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.70002 0 270) (size 3.50012 2.30124) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C3-Pad1)") (zone_connect 2))
    (model SMB_Faktor03937_RevA_06Sep2012.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:SOP-8EP (layer F.Cu) (tedit 5569DA46)
    (at 136.525 120.65)
    (fp_text reference U3 (at 2.286 -4.572) (layer F.SilkS) hide)
    (fp_text value ACT2103 (at 0 -3.175) (layer F.SilkS))
    (pad 4 smd rect (at 0 0) (size 2.413 3.302) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 smd rect (at -3 -1.905) (size 1.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C3-Pad2)"))
    (pad 2 smd rect (at -3 -0.635) (size 1.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 +BATT))
    (pad 3 smd rect (at -3 0.635) (size 1.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C3-Pad1)"))
    (pad 4 smd rect (at -3 1.905) (size 1.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 8 smd rect (at 3 -1.905) (size 1.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(U3-Pad8)"))
    (pad 7 smd rect (at 3 -0.635) (size 1.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(U3-Pad7)"))
    (pad 6 smd rect (at 3 0.635) (size 1.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 5 smd rect (at 3 1.905) (size 1.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(R1-Pad2)"))
    (pad 4 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.635) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 4 thru_hole circle (at 0 -1.27) (size 1.016 1.016) (drill 0.635) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 4 thru_hole circle (at 0 1.27) (size 1.016 1.016) (drill 0.635) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 4 thru_hole circle (at 1.016 -1.27) (size 1.016 1.016) (drill 0.635) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 4 thru_hole circle (at 1.016 0) (size 1.016 1.016) (drill 0.635) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 4 thru_hole circle (at 1.016 1.27) (size 1.016 1.016) (drill 0.635) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 4 thru_hole circle (at -1.016 1.27) (size 1.016 1.016) (drill 0.635) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 4 thru_hole circle (at -1.016 0) (size 1.016 1.016) (drill 0.635) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 4 thru_hole circle (at -1.016 -1.27) (size 1.016 1.016) (drill 0.635) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
  )
  (module DonB:C_0805_HandSoldering (layer F.Cu) (tedit 540A4FBD)
    (at 127.635 144.78)
    (descr "SMT capacitor, 0805")
    (fp_text reference C13 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value 1uF (at 0 2.206) (layer F.SilkS))
    (pad 1 smd rect (at 1.15062 0) (size 1.4986 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 63 sig_in_off))
    (pad 2 smd rect (at -1.15062 0) (size 1.4986 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 13 af_out))
    (model smd/Capacitors/C0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:R_0805_HandSoldering (layer F.Cu) (tedit 540A4C46)
    (at 133.985 144.78 180)
    (descr "Resistor, SMD, 0805, Hand soldering,")
    (tags "Resistor, SMD, 0805, Hand soldering,")
    (attr smd)
    (fp_text reference R14 (at 0 -1.5 180) (layer F.SilkS) hide)
    (fp_text value 100K (at -0.08 1.524 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.30048 0 180) (size 1.50114 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 7 +3.3VP))
    (pad 2 smd rect (at 1.30048 0 180) (size 1.50114 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 63 sig_in_off))
    (model smd/resistors/R0805/R0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:R_0805_HandSoldering (layer F.Cu) (tedit 5569375E)
    (at 133.985 147.955)
    (descr "Resistor, SMD, 0805, Hand soldering,")
    (tags "Resistor, SMD, 0805, Hand soldering,")
    (attr smd)
    (fp_text reference R15 (at 0 -1.5) (layer F.SilkS) hide)
    (fp_text value 100K (at 0 -1.524) (layer F.SilkS))
    (pad 1 smd rect (at -1.30048 0) (size 1.50114 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 63 sig_in_off))
    (pad 2 smd rect (at 1.30048 0) (size 1.50114 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model smd/resistors/R0805/R0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:R_0805_HandSoldering (layer F.Cu) (tedit 540A4C46)
    (at 109.982 133.35 90)
    (descr "Resistor, SMD, 0805, Hand soldering,")
    (tags "Resistor, SMD, 0805, Hand soldering,")
    (attr smd)
    (fp_text reference R18 (at 0 -1.5 90) (layer F.SilkS) hide)
    (fp_text value 4.7K (at -0.08 1.524 90) (layer F.SilkS))
    (pad 1 smd rect (at -1.30048 0 90) (size 1.50114 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 31 rst))
    (pad 2 smd rect (at 1.30048 0 90) (size 1.50114 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 8 +3V3))
    (model smd/resistors/R0805/R0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:TESTPIN (layer F.Cu) (tedit 5569D6C5)
    (at 132.08 111.76)
    (fp_text reference P11 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value Batt (at 0 2.54 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.651 1.651) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 +BATT))
  )
  (module DonB:TESTPIN (layer F.Cu) (tedit 5569D7FD)
    (at 135.89 111.76)
    (fp_text reference P12 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value GND (at 0 2.54 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.651 1.651) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
  )
  (module DonB:NavSpark (layer F.Cu) (tedit 5569DCAD)
    (at 99.314 132.08)
    (fp_text reference U1 (at 3.81 13.97) (layer F.SilkS))
    (fp_text value NavSpark (at -4.572 9.906 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7.62 -15.24) (size 1.651 1.651) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 41 "Net-(U1-Pad1)"))
    (pad 2 thru_hole circle (at -7.62 -12.7) (size 1.651 1.651) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 42 rxNav))
    (pad 3 thru_hole circle (at -7.62 -10.16) (size 1.651 1.651) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 43 txNav))
    (pad 4 thru_hole circle (at -7.62 -7.62) (size 1.651 1.651) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 44 "Net-(U1-Pad4)"))
    (pad 5 thru_hole circle (at -7.62 -5.08) (size 1.651 1.651) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 ptt))
    (pad 6 thru_hole circle (at -7.62 -2.54) (size 1.651 1.651) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 miso))
    (pad 7 thru_hole circle (at -7.62 0) (size 1.651 1.651) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 mosi))
    (pad 8 thru_hole circle (at -7.62 2.54) (size 1.651 1.651) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 57 "Net-(U1-Pad8)"))
    (pad 9 thru_hole circle (at -7.62 5.08) (size 1.651 1.651) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 60 "Net-(U1-Pad9)"))
    (pad 10 thru_hole circle (at -7.62 7.62) (size 1.651 1.651) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 58 "Net-(U1-Pad10)"))
    (pad 11 thru_hole circle (at -7.62 10.16) (size 1.651 1.651) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 45 "Net-(U1-Pad11)"))
    (pad 12 thru_hole circle (at -7.62 12.7) (size 1.651 1.651) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 62 "Net-(U1-Pad12)"))
    (pad 13 thru_hole circle (at -7.62 15.24) (size 1.651 1.651) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 46 "Net-(U1-Pad13)"))
    (pad 14 thru_hole circle (at 7.62 15.24) (size 1.651 1.651) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 47 "Net-(U1-Pad14)"))
    (pad 15 thru_hole circle (at 7.62 12.7) (size 1.651 1.651) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 48 "Net-(U1-Pad15)"))
    (pad 16 thru_hole circle (at 7.62 10.16) (size 1.651 1.651) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 49 serialRadio))
    (pad 17 thru_hole circle (at 7.62 7.62) (size 1.651 1.651) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 50 serial328))
    (pad 18 thru_hole circle (at 7.62 5.08) (size 1.651 1.651) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 37 powerSave))
    (pad 19 thru_hole circle (at 7.62 2.54) (size 1.651 1.651) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 rst))
    (pad 20 thru_hole circle (at 7.62 0) (size 1.651 1.651) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 sck))
    (pad 21 thru_hole circle (at 7.62 -2.54) (size 1.651 1.651) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 59 "Net-(U1-Pad21)"))
    (pad 22 thru_hole circle (at 7.62 -5.08) (size 1.651 1.651) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 23 thru_hole circle (at 7.62 -7.62) (size 1.651 1.651) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 +3V3))
    (pad 24 thru_hole circle (at 7.62 -10.16) (size 1.651 1.651) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 "Net-(U1-Pad24)"))
    (pad 25 thru_hole circle (at 7.62 -12.7) (size 1.651 1.651) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 +BATT))
  )
  (module DonB:Diode-SMB_Handsoldering (layer B.Cu) (tedit 5569FDB7)
    (at 115.57 115.062 90)
    (descr "Diode SMB Handsoldering")
    (tags "Diode SMB Handsoldering")
    (attr smd)
    (fp_text reference D4 (at 0 3 90) (layer B.SilkS) hide)
    (fp_text value SSB43 (at -0.127 -2.159 90) (layer B.SilkS))
    (fp_text user A (at -3.2004 -1.95072 90) (layer B.SilkS))
    (fp_text user K (at 2.99974 -1.95072 90) (layer B.SilkS))
    (pad 1 smd rect (at -2.70002 0 90) (size 3.50012 2.30124) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.70002 0 90) (size 3.50012 2.30124) (layers B.Cu B.Paste B.Mask)
      (net 2 +BATT) (zone_connect 2))
    (model SMB_Faktor03937_RevA_06Sep2012.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Radial_D7.5_L11.2_P2.5 (layer F.Cu) (tedit 556A5C83)
    (at 127.635 113.665 180)
    (descr "Radial Electrolytic Capacitor Diameter 7.5mm x Length 11.2mm, Pitch 2.5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C6 (at 1.25 -5.1 180) (layer F.SilkS))
    (fp_text value 47uF (at 5.969 0 270) (layer F.SilkS))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 +BATT))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D7.5_L11.2_P2.5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:C_0805_HandSoldering (layer F.Cu) (tedit 55981628)
    (at 85.725 146.685 270)
    (descr "SMT capacitor, 0805")
    (fp_text reference C14 (at 4.445 0 270) (layer F.SilkS) hide)
    (fp_text value 2.2nF (at 0 -1.905 270) (layer F.SilkS))
    (pad 1 smd rect (at 1.15062 0 270) (size 1.4986 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 34 mic_out))
    (pad 2 smd rect (at -1.15062 0 270) (size 1.4986 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model smd/Capacitors/C0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text gnd (at 104.521 127) (layer F.SilkS))
  (gr_text mosi (at 94.488 131.953) (layer F.SilkS))
  (gr_text miso (at 94.488 129.413) (layer F.SilkS))
  (gr_text vcc (at 104.521 124.333) (layer F.SilkS))
  (gr_text rst (at 104.648 134.493) (layer F.SilkS))
  (gr_text sck (at 104.521 131.953) (layer F.SilkS))
  (gr_text 74hc4066 (at 99.187 118.872) (layer F.SilkS))
  (gr_text +5-10V (at 131.953 116.078 90) (layer B.SilkS))
  (gr_text GND (at 135.89 114.3 90) (layer B.SilkS))
  (gr_text "Don\nBindner" (at 142.494 143.764) (layer F.SilkS))
  (gr_line (start 147.066 109.728) (end 70.739 109.728) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 149.352 112.014) (end 147.066 109.728) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 149.352 148.717) (end 149.352 112.014) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 148.336 149.733) (end 149.352 148.717) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 69.596 149.733) (end 148.336 149.733) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.453 148.59) (end 69.596 149.733) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.453 112.014) (end 68.453 148.59) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.58 111.887) (end 68.453 112.014) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 70.739 109.728) (end 68.58 111.887) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_text Tx (at 79.883 133.35 90) (layer F.SilkS))
  (gr_text Rx (at 72.136 133.477 90) (layer F.SilkS))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 149.225 123.19) (xy 148.59 123.825) (xy 137.795 123.825) (xy 137.16 123.19) (xy 137.16 112.395)
        (xy 137.795 111.76) (xy 148.59 111.76) (xy 149.225 112.395)
      )
    )
  )
  (zone (net 7) (net_name +3.3VP) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 146.05 133.985) (xy 145.415 134.62) (xy 126.365 134.62) (xy 126.365 129.54) (xy 131.445 129.54)
        (xy 133.985 127) (xy 140.97 127) (xy 142.875 128.905) (xy 145.415 128.905) (xy 146.05 129.54)
      )
    )
  )
  (zone (net 5) (net_name "Net-(C3-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 126.365 121.539) (xy 126.238 121.666) (xy 122.047 121.666) (xy 119.126 124.587) (xy 119.126 134.62)
        (xy 113.792 134.62) (xy 113.792 122.682) (xy 117.348 119.126) (xy 124.714 119.126) (xy 126.365 120.777)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 137.668 126.492) (xy 140.716 126.492) (xy 141.224 125.984) (xy 141.224 124.587) (xy 140.716 124.206)
        (xy 137.541 124.206) (xy 136.906 123.571) (xy 136.906 112.395) (xy 136.271 111.76) (xy 128.524 111.76)
        (xy 128.016 112.268) (xy 128.016 121.539) (xy 127.381 122.174) (xy 122.428 122.174) (xy 120.142 124.46)
        (xy 120.142 124.968) (xy 120.396 125.222) (xy 127.635 125.222) (xy 128.778 126.492) (xy 137.668 126.492)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 149.225 123.19) (xy 148.59 123.825) (xy 137.795 123.825) (xy 137.16 123.19) (xy 137.16 112.395)
        (xy 137.795 111.76) (xy 148.59 111.76) (xy 149.225 112.395)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 126.492 111.506) (xy 127.508 112.522) (xy 127.508 118.618) (xy 116.586 118.618) (xy 113.03 122.174)
        (xy 113.03 138.43) (xy 113.538 138.938) (xy 128.778 138.938) (xy 129.286 138.43) (xy 129.286 135.636)
        (xy 129.794 135.128) (xy 148.59 135.128) (xy 149.352 135.89) (xy 149.352 148.336) (xy 148.336 149.352)
        (xy 69.596 149.352) (xy 68.58 148.336) (xy 68.58 112.268) (xy 70.612 110.236) (xy 125.222 110.236)
        (xy 126.492 111.506)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 149.352 148.336) (xy 148.336 149.352) (xy 69.596 149.352) (xy 68.58 148.336) (xy 68.58 112.268)
        (xy 70.612 110.236) (xy 134.874 110.236) (xy 136.906 112.268) (xy 136.906 123.444) (xy 137.668 124.206)
        (xy 148.59 124.206) (xy 149.352 124.968) (xy 149.352 135.128) (xy 149.352 135.89)
      )
    )
  )
)
