(kicad_pcb (version 4) (host pcbnew 0.201506232253+5814~23~ubuntu14.04.1-product)
  (general
    (links 34)
    (no_connects 0)
    (area 87.63 71.12 167.640001 162.560001)
    (thickness 1.6)
    (drawings 30)
    (tracks 115)
    (zones 0)
    (modules 23)
    (nets 20)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.4986 1.4986)
    (pad_drill 0)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerbers/))
  )
  (net 0 "")
  (net 1 +3.3VP)
  (net 2 GND)
  (net 3 mic_out)
  (net 4 txRadio)
  (net 5 rxRadio)
  (net 6 ptt)
  (net 7 powerSave)
  (net 8 sq)
  (net 9 af_out)
  (net 10 "Net-(R1-Pad1)")
  (net 11 "Net-(U1-Pad15)")
  (net 12 "Net-(U1-Pad14)")
  (net 13 "Net-(U1-Pad13)")
  (net 14 "Net-(U1-Pad11)")
  (net 15 "Net-(U1-Pad4)")
  (net 16 "Net-(U1-Pad2)")
  (net 17 "Net-(C3-Pad1)")
  (net 18 "Net-(C4-Pad1)")
  (net 19 "Net-(C5-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(U1-Pad11)")
    (add_net "Net-(U1-Pad13)")
    (add_net "Net-(U1-Pad14)")
    (add_net "Net-(U1-Pad15)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U1-Pad4)")
    (add_net af_out)
    (add_net mic_out)
    (add_net powerSave)
    (add_net ptt)
    (add_net rxRadio)
    (add_net sq)
    (add_net txRadio)
  )
  (net_class 50ohm ""
    (clearance 0.1524)
    (trace_width 0.7874)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C4-Pad1)")
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 1.016)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3.3VP)
  )
  (module DonB:C_0805_HandSoldering (layer B.Cu) (tedit 5569EC9C)
    (at 139.7 116.84)
    (descr "SMT capacitor, 0805")
    (fp_text reference C1 (at 0 2) (layer B.SilkS) hide)
    (fp_text value 10uF (at 0 1.778) (layer B.SilkS))
    (pad 1 smd rect (at 1.15062 0) (size 1.4986 1.4986) (layers B.Cu B.Paste B.Mask)
      (net 1 +3.3VP))
    (pad 2 smd rect (at -1.15062 0) (size 1.4986 1.4986) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model smd/Capacitors/C0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:SMA-142-0701-201 (layer F.Cu) (tedit 556786A9)
    (at 119.38 109.22)
    (fp_text reference P1 (at 0 5.08) (layer F.SilkS))
    (fp_text value SMA (at 0 -5.08) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 2.54 2.54) (drill 1.5875) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(C3-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 -2.54) (size 2.54 2.54) (drill 1.778) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole circle (at 2.54 2.54) (size 2.54 2.54) (drill 1.778) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole circle (at -2.54 2.54) (size 2.54 2.54) (drill 1.778) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole circle (at -2.54 -2.54) (size 2.54 2.54) (drill 1.778) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module DonB:TESTPIN (layer F.Cu) (tedit 55677B30)
    (at 139.7 83.82)
    (fp_text reference P2 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value mic_out (at 0 2) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.651 1.651) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 mic_out))
  )
  (module DonB:TESTPIN (layer F.Cu) (tedit 55677B2B)
    (at 139.7 86.36)
    (fp_text reference P3 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value txRadio (at 0 2) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.651 1.651) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 txRadio))
  )
  (module DonB:TESTPIN (layer F.Cu) (tedit 55677B35)
    (at 142.24 83.82)
    (fp_text reference P4 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value rxRadio (at 0 2) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.651 1.651) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 rxRadio))
  )
  (module DonB:TESTPIN (layer F.Cu) (tedit 556789B2)
    (at 142.24 86.36)
    (fp_text reference P5 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value GND (at 0 2) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.651 1.651) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND) (zone_connect 2))
  )
  (module DonB:TESTPIN (layer F.Cu) (tedit 55677B41)
    (at 144.78 83.82)
    (fp_text reference P6 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value GND (at 0 2) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.651 1.651) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module DonB:TESTPIN (layer F.Cu) (tedit 55677B45)
    (at 144.78 86.36)
    (fp_text reference P7 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value +3.3V (at 0 2) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.651 1.651) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3.3VP))
  )
  (module DonB:TESTPIN (layer F.Cu) (tedit 55677B4E)
    (at 147.32 83.82)
    (fp_text reference P8 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value ptt (at 0 2) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.651 1.651) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 ptt))
  )
  (module DonB:TESTPIN (layer F.Cu) (tedit 55677B49)
    (at 147.32 86.36)
    (fp_text reference P9 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value powerSave (at 0 2) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.651 1.651) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 powerSave))
  )
  (module DonB:TESTPIN (layer F.Cu) (tedit 55677B5B)
    (at 149.86 83.82)
    (fp_text reference P10 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value sq (at 0 2) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.651 1.651) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 sq))
  )
  (module DonB:TESTPIN (layer F.Cu) (tedit 55677B56)
    (at 149.86 86.36)
    (fp_text reference P11 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value af_out (at 0 2) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.651 1.651) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 af_out))
  )
  (module DonB:R_0805_HandSoldering (layer B.Cu) (tedit 55678258)
    (at 149.225 118.11 90)
    (descr "Resistor, SMD, 0805, Hand soldering,")
    (tags "Resistor, SMD, 0805, Hand soldering,")
    (attr smd)
    (fp_text reference R1 (at 0 -1.651 90) (layer B.SilkS) hide)
    (fp_text value 0R (at 0 1.905 90) (layer B.SilkS))
    (pad 1 smd rect (at -1.30048 0 90) (size 1.50114 1.19888) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(R1-Pad1)"))
    (pad 2 smd rect (at 1.30048 0 90) (size 1.50114 1.19888) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model smd/resistors/R0805/R0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:C_0805_HandSoldering (layer B.Cu) (tedit 5569ECA0)
    (at 139.7 120.65)
    (descr "SMT capacitor, 0805")
    (fp_text reference C2 (at 0 -1.905) (layer B.SilkS) hide)
    (fp_text value 100nF (at 0 1.778) (layer B.SilkS))
    (pad 1 smd rect (at 1.15062 0) (size 1.4986 1.4986) (layers B.Cu B.Paste B.Mask)
      (net 1 +3.3VP))
    (pad 2 smd rect (at -1.15062 0) (size 1.4986 1.4986) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model smd/Capacitors/C0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:PAD-3.35mm (layer F.Cu) (tedit 5589FF3C)
    (at 116.84 127)
    (fp_text reference P12 (at 0 -3) (layer F.SilkS) hide)
    (fp_text value GND (at -0.635 -3.175) (layer F.SilkS))
    (pad 1 smd rect (at 0 0) (size 3.35 3.35) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module DonB:PAD-3.35mm (layer F.Cu) (tedit 5569F4CC)
    (at 116.84 91.44)
    (fp_text reference P13 (at 0 -3) (layer F.SilkS) hide)
    (fp_text value GND (at 0 3.302) (layer F.SilkS))
    (pad 1 smd rect (at 0 0) (size 3.35 3.35) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module DonB:C_0805_HandSoldering (layer F.Cu) (tedit 558B3BB1)
    (at 125.73 120.015 180)
    (descr "SMT capacitor, 0805")
    (fp_text reference C3 (at 0 -2 180) (layer F.SilkS) hide)
    (fp_text value 20pF (at 4.064 0.381 180) (layer F.SilkS))
    (pad 1 smd rect (at 1.15062 0 180) (size 1.4986 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at -1.15062 0 180) (size 1.4986 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model smd/Capacitors/C0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:C_0805_HandSoldering (layer F.Cu) (tedit 558B3BAC)
    (at 125.73 125.095)
    (descr "SMT capacitor, 0805")
    (fp_text reference C4 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value 20pF (at -4.064 0.381) (layer F.SilkS))
    (pad 1 smd rect (at 1.15062 0) (size 1.4986 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at -1.15062 0) (size 1.4986 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model smd/Capacitors/C0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:C_0805_HandSoldering (layer F.Cu) (tedit 558A0FD3)
    (at 125.73 122.555 180)
    (descr "SMT capacitor, 0805")
    (fp_text reference L1 (at 0 -2 180) (layer F.SilkS) hide)
    (fp_text value 56nH (at 4.064 -0.127 180) (layer F.SilkS))
    (pad 1 smd rect (at 1.15062 0 180) (size 1.4986 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at -1.15062 0 180) (size 1.4986 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C4-Pad1)"))
    (model smd/Capacitors/C0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:R_0805_HandSoldering (layer B.Cu) (tedit 559145C1)
    (at 140.97 100.33 180)
    (descr "Resistor, SMD, 0805, Hand soldering,")
    (tags "Resistor, SMD, 0805, Hand soldering,")
    (attr smd)
    (fp_text reference R2 (at -3.81 0 180) (layer B.SilkS) hide)
    (fp_text value P/U (at 0 -1.905 180) (layer B.SilkS))
    (pad 1 smd rect (at -1.30048 0 180) (size 1.50114 1.19888) (layers B.Cu B.Paste B.Mask)
      (net 1 +3.3VP))
    (pad 2 smd rect (at 1.30048 0 180) (size 1.50114 1.19888) (layers B.Cu B.Paste B.Mask)
      (net 19 "Net-(C5-Pad1)"))
    (model smd/resistors/R0805/R0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:C_0805_HandSoldering (layer F.Cu) (tedit 540A4FBD)
    (at 135.255 85.725 270)
    (descr "SMT capacitor, 0805")
    (fp_text reference C5 (at 0 -2 270) (layer F.SilkS) hide)
    (fp_text value 1uF (at 0 2.206 270) (layer F.SilkS))
    (pad 1 smd rect (at 1.15062 0 270) (size 1.4986 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at -1.15062 0 270) (size 1.4986 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 3 mic_out))
    (model smd/Capacitors/C0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:R_0805_HandSoldering (layer B.Cu) (tedit 559145BE)
    (at 134.62 100.33 180)
    (descr "Resistor, SMD, 0805, Hand soldering,")
    (tags "Resistor, SMD, 0805, Hand soldering,")
    (attr smd)
    (fp_text reference R3 (at 3.175 0 180) (layer B.SilkS) hide)
    (fp_text value P/D (at 0 -1.905 180) (layer B.SilkS))
    (pad 1 smd rect (at -1.30048 0 180) (size 1.50114 1.19888) (layers B.Cu B.Paste B.Mask)
      (net 19 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 1.30048 0 180) (size 1.50114 1.19888) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model smd/resistors/R0805/R0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:DRA818 (layer F.Cu) (tedit 55913CFA)
    (at 144.78 109.22)
    (fp_text reference U1 (at 0 -14.605) (layer F.SilkS))
    (fp_text value DRA818 (at 0 13.97) (layer F.SilkS))
    (fp_text user 18 (at -8 -16) (layer F.SilkS))
    (fp_text user 1 (at 8 -16) (layer F.SilkS))
    (pad 18 smd rect (at -8.6 -13.35) (size 5.4 1.8) (drill (offset -1.8 0)) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(C5-Pad1)"))
    (pad 17 smd rect (at -8.6 -8.9) (size 5.4 1.8) (drill (offset -1.8 0)) (layers F.Cu F.Paste F.Mask)
      (net 4 txRadio))
    (pad 16 smd rect (at -8.6 -4.45) (size 5.4 1.8) (drill (offset -1.8 0)) (layers F.Cu F.Paste F.Mask)
      (net 5 rxRadio))
    (pad 15 smd rect (at -8.6 0) (size 5.4 1.8) (drill (offset -1.8 0)) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(U1-Pad15)"))
    (pad 14 smd rect (at -8.6 4.45) (size 5.4 1.8) (drill (offset -1.8 0)) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(U1-Pad14)"))
    (pad 13 smd rect (at -8.6 8.9) (size 5.4 1.8) (drill (offset -1.8 0)) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(U1-Pad13)"))
    (pad 12 smd rect (at -8.6 13.35) (size 5.4 1.8) (drill (offset -1.8 0)) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C4-Pad1)"))
    (pad 11 smd rect (at -6.9 16.9) (size 1.8 5.4) (drill (offset 0 1.8)) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(U1-Pad11)"))
    (pad 10 smd rect (at -2.3 16.9) (size 1.8 5.4) (drill (offset 0 1.8)) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 9 smd rect (at 2.3 16.9) (size 1.8 5.4) (drill (offset 0 1.8)) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 8 smd rect (at 6.9 16.9) (size 1.8 5.4) (drill (offset 0 1.8)) (layers F.Cu F.Paste F.Mask)
      (net 1 +3.3VP))
    (pad 7 smd rect (at 8.6 13.35) (size 5.4 1.8) (drill (offset 1.8 0)) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(R1-Pad1)"))
    (pad 6 smd rect (at 8.6 8.9) (size 5.4 1.8) (drill (offset 1.8 0)) (layers F.Cu F.Paste F.Mask)
      (net 7 powerSave))
    (pad 5 smd rect (at 8.6 4.45) (size 5.4 1.8) (drill (offset 1.8 0)) (layers F.Cu F.Paste F.Mask)
      (net 6 ptt))
    (pad 4 smd rect (at 8.6 0) (size 5.4 1.8) (drill (offset 1.8 0)) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(U1-Pad4)"))
    (pad 3 smd rect (at 8.6 -4.45) (size 5.4 1.8) (drill (offset 1.8 0)) (layers F.Cu F.Paste F.Mask)
      (net 9 af_out))
    (pad 2 smd rect (at 8.6 -8.9) (size 5.4 1.8) (drill (offset 1.8 0)) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(U1-Pad2)"))
    (pad 1 smd rect (at 8.6 -13.35) (size 5.4 1.8) (drill (offset 1.8 0)) (layers F.Cu F.Paste F.Mask)
      (net 8 sq))
  )
  (gr_line (start 157.988 131.318) (end 158.115 131.318) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 157.988 81.28) (end 158.115 81.28) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 158.623 130.556) (end 158.623 130.81) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.49 130.556) (end 110.49 130.81) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 158.623 130.556) (end 158.623 111.506) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 157.988 131.318) (end 115.824 131.318) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 158.623 130.81) (end 158.115 131.318) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.49 130.81) (end 110.998 131.318) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.49 87.884) (end 110.49 130.556) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 129.54 87.376) (end 110.998 87.376) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.49 87.884) (end 110.998 87.376) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 158.623 81.788) (end 158.623 111.506) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 158.115 81.28) (end 158.623 81.788) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 130.556 81.28) (end 157.988 81.28) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 130.302 81.534) (end 130.556 81.28) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 130.048 81.788) (end 130.302 81.534) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 130.048 86.868) (end 130.048 81.788) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 129.54 87.376) (end 130.048 86.868) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.824 131.318) (end 110.998 131.318) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_text "Don Bindner" (at 156.21 113.03 90) (layer B.SilkS))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 167.64 162.56) (xy 87.63 162.56) (xy 87.63 71.12) (xy 167.64 71.12)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 167.64 162.56) (xy 87.63 162.56) (xy 87.63 71.12) (xy 167.64 71.12)
      )
    )
  )
)
