(module Don-FET-GDS-horiz (layer F.Cu) (tedit 540A4BB6)
  (descr "TO-220, FET-GDS, Horizontal,")
  (tags "TO-220, FET-GDS, Horizontal,")
  (fp_text reference Q1 (at -0.09906 -21.99894) (layer F.SilkS))
  (fp_text value IRF4905 (at 0 3.5) (layer F.SilkS) hide)
  (fp_text user S (at 2.54 -5.08) (layer F.SilkS))
  (fp_text user D (at 0 -5.08) (layer F.SilkS))
  (fp_text user G (at -2.54 -5.08) (layer F.SilkS))
  (pad D thru_hole oval (at 0 0 90) (size 2.49936 1.50114) (drill 1.00076) (layers *.Cu *.Mask F.SilkS))
  (pad G thru_hole oval (at -2.54 0 90) (size 2.49936 1.50114) (drill 1.00076) (layers *.Cu *.Mask F.SilkS))
  (pad S thru_hole oval (at 2.54 0 90) (size 2.49936 1.50114) (drill 1.00076) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 -16.764 90) (size 3.79984 3.79984) (drill 3.79984) (layers *.Cu *.Mask F.SilkS))
  (pad D smd rect (at 0 -12.5) (size 9 12) (drill (offset 0 -2)) (layers F.Cu F.Paste F.Mask)
    (zone_connect 2))
  (model Transistor_TO-220_Wings3d_RevB_03Sep2012/TO220-Horizontal_RevB_Faktor03937_03Sep2012.wrl
    (at (xyz 0 0 0))
    (scale (xyz 0.3937 0.3937 0.3937))
    (rotate (xyz 0 0 0))
  )
)
