(module MicroFTX (layer F.Cu) (tedit 54976ED6)
  (fp_text reference MicroFTX (at 0 10.16) (layer F.SilkS))
  (fp_text value VAL** (at 0 0) (layer F.SilkS) hide)
  (fp_text user + (at 3.048 5.08) (layer F.SilkS))
  (fp_text user RX (at 1.27 5.08) (layer F.SilkS))
  (fp_text user TX (at -1.27 5.08) (layer F.SilkS))
  (fp_text user - (at -2.794 5.08) (layer F.SilkS))
  (fp_text user RTS (at 1.524 3.556) (layer F.SilkS))
  (fp_text user CTS (at 1.524 1.016) (layer F.SilkS))
  (fp_text user CB2 (at 1.524 -1.524) (layer F.SilkS))
  (fp_text user CB3 (at -1.27 3.556) (layer F.SilkS))
  (fp_text user CB0 (at -1.27 1.016) (layer F.SilkS))
  (fp_text user CB1 (at -1.27 -1.524) (layer F.SilkS))
  (pad 8 thru_hole circle (at -3.81 -1.27) (size 1.524 1.524) (drill 1) (layers *.Cu *.Mask F.SilkS))
  (pad 9 thru_hole circle (at -3.81 1.27) (size 1.524 1.524) (drill 1) (layers *.Cu *.Mask F.SilkS))
  (pad 10 thru_hole circle (at -3.81 3.81) (size 1.524 1.524) (drill 1) (layers *.Cu *.Mask F.SilkS))
  (pad 11 thru_hole circle (at -3.81 6.35) (size 1.524 1.524) (drill 1) (layers *.Cu *.Mask F.SilkS))
  (pad 12 thru_hole circle (at -1.27 6.35) (size 1.524 1.524) (drill 1) (layers *.Cu *.Mask F.SilkS))
  (pad 13 thru_hole circle (at 1.27 6.35) (size 1.524 1.524) (drill 1) (layers *.Cu *.Mask F.SilkS))
  (pad 14 thru_hole circle (at 3.81 6.35) (size 1.524 1.524) (drill 1) (layers *.Cu *.Mask F.SilkS))
  (pad 15 thru_hole circle (at 3.81 3.81) (size 1.524 1.524) (drill 1) (layers *.Cu *.Mask F.SilkS))
  (pad 16 thru_hole circle (at 3.81 1.27) (size 1.524 1.524) (drill 1) (layers *.Cu *.Mask F.SilkS))
  (pad 17 thru_hole circle (at 3.81 -1.27) (size 1.524 1.524) (drill 1) (layers *.Cu *.Mask F.SilkS))
)
