(kicad_pcb (version 4) (host pcbnew 0.201511192131+6326~38~ubuntu14.04.1-stable)
  (general
    (links 68)
    (no_connects 0)
    (area 78.2733 95.25 147.320001 116.840001)
    (thickness 1.6)
    (drawings 10)
    (tracks 293)
    (zones 0)
    (modules 33)
    (nets 31)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.254)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.127000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerbers))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(C1-Pad2)")
  (net 3 "Net-(C2-Pad2)")
  (net 4 "Net-(C3-Pad2)")
  (net 5 +9V)
  (net 6 "Net-(C4-Pad2)")
  (net 7 "Net-(C6-Pad1)")
  (net 8 "Net-(C6-Pad2)")
  (net 9 +3V3)
  (net 10 "Net-(C12-Pad1)")
  (net 11 rst)
  (net 12 test)
  (net 13 "Net-(U2-Pad15)")
  (net 14 shutdown)
  (net 15 "Net-(U2-Pad2)")
  (net 16 "Net-(U2-Pad3)")
  (net 17 "Net-(U2-Pad5)")
  (net 18 "Net-(U2-Pad11)")
  (net 19 "Net-(U2-Pad12)")
  (net 20 "Net-(U2-Pad13)")
  (net 21 "Net-(U2-Pad14)")
  (net 22 gpio1)
  (net 23 "Net-(U2-Pad7)")
  (net 24 gpio0)
  (net 25 "Net-(U2-Pad16)")
  (net 26 "Net-(U2-Pad17)")
  (net 27 "Net-(U3-Pad12)")
  (net 28 "Net-(U2-Pad19)")
  (net 29 gpio3)
  (net 30 "Net-(R3-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +9V)
    (add_net GND)
    (add_net "Net-(C12-Pad1)")
    (add_net "Net-(C4-Pad2)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(U2-Pad11)")
    (add_net "Net-(U2-Pad12)")
    (add_net "Net-(U2-Pad13)")
    (add_net "Net-(U2-Pad14)")
    (add_net "Net-(U2-Pad15)")
    (add_net "Net-(U2-Pad16)")
    (add_net "Net-(U2-Pad17)")
    (add_net "Net-(U2-Pad19)")
    (add_net "Net-(U2-Pad2)")
    (add_net "Net-(U2-Pad3)")
    (add_net "Net-(U2-Pad5)")
    (add_net "Net-(U2-Pad7)")
    (add_net "Net-(U3-Pad12)")
    (add_net gpio0)
    (add_net gpio1)
    (add_net gpio3)
    (add_net rst)
    (add_net shutdown)
    (add_net test)
  )
  (net_class 50ohm ""
    (clearance 0.1524)
    (trace_width 0.7874)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C6-Pad2)")
  )
  (module DonB:SOT23_Handsoldering (layer B.Cu) (tedit 565154B9)
    (at 109.22 100.33)
    (descr "Diode, SOT23, Handsoldering, RevA, 03Aug2010,")
    (tags "Diode, SOT23, Handsoldering, RevA, 03Aug2010,")
    (attr smd)
    (fp_text reference D1 (at 0 3.175) (layer B.SilkS))
    (fp_text value PMEG2010 (at 0 -3.81) (layer B.SilkS) hide)
    (pad 1 smd rect (at -1 -1.50114) (size 0.8001 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 5 +9V))
    (pad 2 smd rect (at 1 -1.50114) (size 0.8001 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 5 +9V))
    (pad 3 smd rect (at 0 1.50114) (size 0.8001 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(C4-Pad2)"))
  )
  (module DonB:C_0805_HandSoldering (layer F.Cu) (tedit 564DDF44)
    (at 95.25 107.95 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 3.556 0 90) (layer F.SilkS))
    (fp_text value 22pF (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:C_0805_HandSoldering (layer F.Cu) (tedit 564EB722)
    (at 102.87 107.95 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 4.445 0 90) (layer F.SilkS))
    (fp_text value 39pF (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:C_0805_HandSoldering (layer F.Cu) (tedit 564EB780)
    (at 110.49 107.95 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at 4.445 0 90) (layer F.SilkS))
    (fp_text value 22pF (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:C_0805_HandSoldering (layer B.Cu) (tedit 565154AF)
    (at 105.41 100.33 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at 3.175 0 360) (layer B.SilkS))
    (fp_text value 10nF (at 0 0 270) (layer B.SilkS) hide)
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 5 +9V))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(C4-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:C_0805_HandSoldering (layer B.Cu) (tedit 5651574A)
    (at 113.03 100.33 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at -3.175 0 180) (layer B.SilkS))
    (fp_text value 1uF (at 0 0 90) (layer B.SilkS) hide)
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(C4-Pad2)"))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:C_0805_HandSoldering (layer F.Cu) (tedit 564EB759)
    (at 119.38 106.68 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C6 (at -0.635 1.651 180) (layer F.SilkS))
    (fp_text value 12pF (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C6-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:C_0805_HandSoldering (layer F.Cu) (tedit 5651581F)
    (at 116.84 100.33 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C7 (at 0.127 1.905 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 9 +3V3))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:C_0805_HandSoldering (layer F.Cu) (tedit 564EB760)
    (at 118.11 113.03 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C8 (at -3.302 0 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 9 +3V3))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:C_0805_HandSoldering (layer F.Cu) (tedit 564EB762)
    (at 120.65 113.03 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C9 (at -3.302 0 270) (layer F.SilkS))
    (fp_text value 1nF (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 9 +3V3))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:C_0805_HandSoldering (layer F.Cu) (tedit 564EB765)
    (at 123.19 113.03 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C10 (at -3.556 0 270) (layer F.SilkS))
    (fp_text value 100pF (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 9 +3V3))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:C_0805_HandSoldering (layer B.Cu) (tedit 56515E58)
    (at 121.92 98.425)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C11 (at 0 1.905 180) (layer B.SilkS))
    (fp_text value 1uF (at -0.127 0.127) (layer B.SilkS) hide)
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 9 +3V3))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:C_0805_HandSoldering (layer F.Cu) (tedit 564DDC38)
    (at 128.27 113.03 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C12 (at 0 -2.1 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C12-Pad1)"))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:C_0805_HandSoldering (layer F.Cu) (tedit 564DCB9F)
    (at 137.16 100.33 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C13 (at -3.81 0 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 9 +3V3))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:C_0805_HandSoldering (layer F.Cu) (tedit 564DDC41)
    (at 137.16 113.03)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C14 (at 3.81 0) (layer F.SilkS))
    (fp_text value 1nF (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 11 rst))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:R_0805_HandSoldering (layer F.Cu) (tedit 564EB748)
    (at 99.06 106.68 180)
    (descr "Resistor, SMD, 0805, Hand soldering,")
    (tags "Resistor, SMD, 0805, Hand soldering,")
    (attr smd)
    (fp_text reference L1 (at 0 2.921 180) (layer F.SilkS))
    (fp_text value 68nH (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.30048 0 180) (size 1.50114 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad2)"))
    (pad 2 smd rect (at 1.30048 0 180) (size 1.50114 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model smd/resistors/R0805/R0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:R_0805_HandSoldering (layer F.Cu) (tedit 56512D3E)
    (at 106.68 106.68 180)
    (descr "Resistor, SMD, 0805, Hand soldering,")
    (tags "Resistor, SMD, 0805, Hand soldering,")
    (attr smd)
    (fp_text reference L2 (at 0 2.921 180) (layer F.SilkS))
    (fp_text value 68nH (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.30048 0 180) (size 1.50114 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad2)"))
    (pad 2 smd rect (at 1.30048 0 180) (size 1.50114 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad2)"))
    (model smd/resistors/R0805/R0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:R_0805_HandSoldering (layer F.Cu) (tedit 56512D52)
    (at 114.3 106.68 180)
    (descr "Resistor, SMD, 0805, Hand soldering,")
    (tags "Resistor, SMD, 0805, Hand soldering,")
    (attr smd)
    (fp_text reference L3 (at 0 2.921 180) (layer F.SilkS))
    (fp_text value 100nH (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.30048 0 180) (size 1.50114 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C6-Pad2)"))
    (pad 2 smd rect (at 1.30048 0 180) (size 1.50114 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad2)"))
    (model smd/resistors/R0805/R0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:R_1210_HandSoldering (layer F.Cu) (tedit 564DDBD7)
    (at 120.65 100.33 90)
    (descr "Resistor SMD 1210, hand soldering")
    (tags "resistor 1210")
    (attr smd)
    (fp_text reference L4 (at 0 2.54 90) (layer F.SilkS))
    (fp_text value 1uH (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2 0 90) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at 2 0 90) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 9 +3V3))
    (model Resistors_SMD.3dshapes/R_1210_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:SMA-142-0701-0801 (layer F.Cu) (tedit 56510C6A)
    (at 90.17 106.68 90)
    (fp_text reference P1 (at 7.62 0 90) (layer F.SilkS) hide)
    (fp_text value BNC (at 0 -10.795 90) (layer F.Fab))
    (pad 2 thru_hole circle (at -4.3815 3.429 90) (size 0.7112 0.7112) (drill 0.4572) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 smd rect (at -4.3815 2.54 90) (size 0.4572 0.889) (drill (offset 0 0.4445)) (layers *.Cu *.Paste *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 smd rect (at -4.3815 0 90) (size 2.413 5.08) (layers *.Cu *.Paste *.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0 0 90) (size 2.286 5.08) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 2 smd rect (at 4.3815 0 90) (size 2.413 5.08) (layers *.Cu *.Paste *.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 4.3815 2.54 90) (size 0.4572 0.889) (drill (offset 0 0.4445)) (layers *.Cu *.Paste *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 4.3815 3.429 90) (size 0.7112 0.7112) (drill 0.4572) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
  )
  (module DonB:TESTPIN (layer B.Cu) (tedit 56512848)
    (at 144.78 101.6)
    (fp_text reference P2 (at 0 2) (layer B.SilkS) hide)
    (fp_text value Vcc (at -2.667 0) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.651 1.651) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 9 +3V3))
  )
  (module DonB:TESTPIN (layer B.Cu) (tedit 5651283E)
    (at 144.78 104.14)
    (fp_text reference P3 (at 0 2) (layer B.SilkS) hide)
    (fp_text value GND (at -2.667 0) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.651 1.651) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 1 GND))
  )
  (module DonB:TESTPIN (layer B.Cu) (tedit 56512841)
    (at 144.78 106.68)
    (fp_text reference P4 (at 0 2) (layer B.SilkS) hide)
    (fp_text value TEST (at -2.667 0) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.651 1.651) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 12 test))
  )
  (module DonB:TESTPIN (layer B.Cu) (tedit 56512846)
    (at 144.78 109.22)
    (fp_text reference P5 (at 0 2) (layer B.SilkS) hide)
    (fp_text value RST (at -2.667 0) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.651 1.651) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 11 rst))
  )
  (module DonB:R_0805_HandSoldering (layer F.Cu) (tedit 564DDC33)
    (at 125.73 113.03 270)
    (descr "Resistor, SMD, 0805, Hand soldering,")
    (tags "Resistor, SMD, 0805, Hand soldering,")
    (attr smd)
    (fp_text reference R1 (at -3.302 0.762 270) (layer F.SilkS))
    (fp_text value 47R (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.30048 0 270) (size 1.50114 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C12-Pad1)"))
    (pad 2 smd rect (at 1.30048 0 270) (size 1.50114 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 9 +3V3))
    (model smd/resistors/R0805/R0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:R_0805_HandSoldering (layer F.Cu) (tedit 564DDC45)
    (at 137.16 110.49)
    (descr "Resistor, SMD, 0805, Hand soldering,")
    (tags "Resistor, SMD, 0805, Hand soldering,")
    (attr smd)
    (fp_text reference R2 (at 3.81 0) (layer F.SilkS))
    (fp_text value 47K (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.30048 0) (size 1.50114 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 9 +3V3))
    (pad 2 smd rect (at 1.30048 0) (size 1.50114 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 11 rst))
    (model smd/resistors/R0805/R0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:SOT23_Handsoldering (layer B.Cu) (tedit 56515759)
    (at 116.84 100.33)
    (descr "Diode, SOT23, Handsoldering, RevA, 03Aug2010,")
    (tags "Diode, SOT23, Handsoldering, RevA, 03Aug2010,")
    (attr smd)
    (fp_text reference U1 (at -0.127 3.429) (layer B.SilkS))
    (fp_text value NCP1703 (at 0 -3.81) (layer B.SilkS) hide)
    (pad 1 smd rect (at -1 -1.50114) (size 0.8001 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1 -1.50114) (size 0.8001 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 9 +3V3))
    (pad 3 smd rect (at 0 1.50114) (size 0.8001 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(C4-Pad2)"))
  )
  (module Housings_SSOP:TSSOP-14_4.4x5mm_Pitch0.65mm (layer F.Cu) (tedit 565148C1)
    (at 137.16 105.41)
    (descr "14-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U3 (at 0 0.762) (layer F.SilkS))
    (fp_text value MSP430G2211 (at 3.81 0 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -2.95 -1.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 9 +3V3))
    (pad 2 smd rect (at -2.95 -1.3) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 14 shutdown))
    (pad 3 smd rect (at -2.95 -0.65) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(U2-Pad15)"))
    (pad 4 smd rect (at -2.95 0) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(U2-Pad14)"))
    (pad 5 smd rect (at -2.95 0.65) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(U2-Pad13)"))
    (pad 6 smd rect (at -2.95 1.3) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(U2-Pad12)"))
    (pad 7 smd rect (at -2.95 1.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(U2-Pad11)"))
    (pad 8 smd rect (at 2.95 1.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 24 gpio0))
    (pad 9 smd rect (at 2.95 1.3) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 22 gpio1))
    (pad 10 smd rect (at 2.95 0.65) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 11 rst))
    (pad 11 smd rect (at 2.95 0) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 12 test))
    (pad 12 smd rect (at 2.95 -0.65) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(U3-Pad12)"))
    (pad 13 smd rect (at 2.95 -1.3) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(R3-Pad2)"))
    (pad 14 smd rect (at 2.95 -1.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Housings_SSOP.3dshapes/TSSOP-14_4.4x5mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:CRYSTAL-3.2x2.5 (layer F.Cu) (tedit 564DCAEF)
    (at 128.27 99.06)
    (fp_text reference Y1 (at 3.81 0) (layer F.SilkS))
    (fp_text value 30MHz (at 0 0) (layer F.Fab))
    (pad 4 smd rect (at -1.15 -0.925) (size 1.9 1.2) (drill (offset -0.5 -0.075)) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 1.15 0.925) (size 1.9 1.2) (drill (offset 0.5 0.075)) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -1.15 0.925) (size 1.9 1.2) (drill (offset -0.5 0.075)) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(U2-Pad17)"))
    (pad 2 smd rect (at 1.15 -0.925) (size 1.9 1.2) (drill (offset 0.5 -0.075)) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(U2-Pad16)"))
  )
  (module DonB:TESTPIN (layer B.Cu) (tedit 564DCC01)
    (at 96.52 100.33 270)
    (fp_text reference P6 (at 0 2 270) (layer B.SilkS) hide)
    (fp_text value GND (at 3.81 0 270) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.651 1.651) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 1 GND))
  )
  (module DonB:TESTPIN (layer B.Cu) (tedit 564DCBFF)
    (at 101.6 100.33 270)
    (fp_text reference P7 (at 0 2 270) (layer B.SilkS) hide)
    (fp_text value 4-16V (at 3.81 0 270) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.651 1.651) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 5 +9V))
  )
  (module DonB:R_0805_HandSoldering (layer B.Cu) (tedit 5652053C)
    (at 127.762 102.235)
    (descr "Resistor, SMD, 0805, Hand soldering,")
    (tags "Resistor, SMD, 0805, Hand soldering,")
    (attr smd)
    (fp_text reference R3 (at 0 -1.651) (layer B.SilkS))
    (fp_text value 47R (at 0 0) (layer B.SilkS) hide)
    (pad 1 smd rect (at -1.30048 0) (size 1.50114 1.19888) (layers B.Cu B.Paste B.Mask)
      (net 29 gpio3))
    (pad 2 smd rect (at 1.30048 0) (size 1.50114 1.19888) (layers B.Cu B.Paste B.Mask)
      (net 30 "Net-(R3-Pad2)"))
    (model smd/resistors/R0805/R0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:QFN-20-1EP_HandSoldering (layer F.Cu) (tedit 56527F9B)
    (at 127 106.045)
    (attr smd)
    (fp_text reference U2 (at 2.54 3.048) (layer F.SilkS))
    (fp_text value Si406x (at 0 0.635) (layer F.SilkS) hide)
    (pad 15 smd rect (at 2 -1) (size 1.5 0.25) (drill (offset 0.33 0)) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(U2-Pad15)"))
    (pad 1 smd rect (at -2 -1) (size 1.5 0.25) (drill (offset -0.33 0)) (layers F.Cu F.Paste F.Mask)
      (net 14 shutdown))
    (pad 2 smd rect (at -2 -0.5) (size 1.5 0.25) (drill (offset -0.33 0)) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(U2-Pad2)"))
    (pad 3 smd rect (at -2 0) (size 1.5 0.25) (drill (offset -0.33 0)) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(U2-Pad3)"))
    (pad 4 smd rect (at -2 0.5) (size 1.5 0.25) (drill (offset -0.33 0)) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C6-Pad1)"))
    (pad 5 smd rect (at -2 1) (size 1.5 0.25) (drill (offset -0.33 0)) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(U2-Pad5)"))
    (pad 11 smd rect (at 2 1) (size 1.5 0.25) (drill (offset 0.33 0)) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(U2-Pad11)"))
    (pad 12 smd rect (at 2 0.5) (size 1.5 0.25) (drill (offset 0.33 0)) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(U2-Pad12)"))
    (pad 13 smd rect (at 2 0) (size 1.5 0.25) (drill (offset 0.33 0)) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(U2-Pad13)"))
    (pad 14 smd rect (at 2 -0.5) (size 1.5 0.25) (drill (offset 0.33 0)) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(U2-Pad14)"))
    (pad 10 smd rect (at 1 2 90) (size 1.5 0.25) (drill (offset -0.33 0)) (layers F.Cu F.Paste F.Mask)
      (net 22 gpio1))
    (pad 21 smd trapezoid (at 0 0) (size 2.6 2.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 6 smd rect (at -1 2 90) (size 1.5 0.25) (drill (offset -0.33 0)) (layers F.Cu F.Paste F.Mask)
      (net 9 +3V3))
    (pad 7 smd rect (at -0.5 2 90) (size 1.5 0.25) (drill (offset -0.33 0)) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(U2-Pad7)"))
    (pad 8 smd rect (at 0 2 90) (size 1.5 0.25) (drill (offset -0.33 0)) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C12-Pad1)"))
    (pad 9 smd rect (at 0.5 2 90) (size 1.5 0.25) (drill (offset -0.33 0)) (layers F.Cu F.Paste F.Mask)
      (net 24 gpio0))
    (pad 16 smd rect (at 1 -2 90) (size 1.5 0.25) (drill (offset 0.33 0)) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(U2-Pad16)"))
    (pad 17 smd rect (at 0.5 -2 90) (size 1.5 0.25) (drill (offset 0.33 0)) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(U2-Pad17)"))
    (pad 18 smd rect (at 0 -2 90) (size 1.5 0.25) (drill (offset 0.33 0)) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 19 smd rect (at -0.5 -2 90) (size 1.5 0.25) (drill (offset 0.33 0)) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(U2-Pad19)"))
    (pad 20 smd rect (at -1 -2 90) (size 1.5 0.25) (drill (offset 0.33 0)) (layers F.Cu F.Paste F.Mask)
      (net 29 gpio3))
  )
  (gr_arc (start 88.392 97.536) (end 87.376 97.536) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 88.392 114.808) (end 88.392 115.824) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 145.288 114.808) (end 146.304 114.808) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 145.288 97.536) (end 145.288 96.52) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "Don Bindner" (at 104.775 113.411) (layer F.SilkS))
  (gr_line (start 87.376 114.808) (end 87.376 104.648) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 145.288 115.824) (end 88.392 115.824) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 146.304 97.536) (end 146.304 114.808) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 88.392 96.52) (end 145.288 96.52) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 87.376 104.648) (end 87.376 97.536) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 86.36 95.25) (xy 147.32 95.25) (xy 147.32 116.84) (xy 86.36 116.84)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 86.36 95.25) (xy 147.32 95.25) (xy 147.32 116.84) (xy 86.36 116.84)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 125.476 97.282) (xy 131.064 97.282) (xy 131.064 100.838) (xy 125.476 100.838)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 119.38 99.314) (xy 121.92 99.314) (xy 121.92 101.346) (xy 119.38 101.346)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 125.857 104.902) (xy 128.143 104.902) (xy 128.143 107.188) (xy 125.857 107.188)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 106.299 105.918) (xy 107.061 105.918) (xy 107.061 107.442) (xy 106.299 107.442)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 98.679 105.918) (xy 99.441 105.918) (xy 99.441 107.442) (xy 98.679 107.442)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.681 107.442) (xy 113.919 107.442) (xy 113.919 105.918) (xy 114.681 105.918) (xy 114.681 107.442)
      )
    )
  )
)
