(kicad_pcb (version 4) (host pcbnew 0.201508030901+6040~28~ubuntu14.04.1-product)
  (general
    (links 71)
    (no_connects 0)
    (area 95.59731 82.608809 172.279953 100.605001)
    (thickness 1.6)
    (drawings 6)
    (tracks 214)
    (zones 0)
    (modules 39)
    (nets 25)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFEFFF)
    (pcbplotparams
      (layerselection 0x010fc_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerbers/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +9V)
  (net 3 "Net-(C2-Pad2)")
  (net 4 "Net-(C3-Pad1)")
  (net 5 "Net-(C4-Pad2)")
  (net 6 +3V3)
  (net 7 "Net-(C6-Pad2)")
  (net 8 "Net-(C8-Pad1)")
  (net 9 "Net-(C8-Pad2)")
  (net 10 "Net-(C9-Pad2)")
  (net 11 "Net-(C10-Pad2)")
  (net 12 RST)
  (net 13 VDD)
  (net 14 "Net-(L2-Pad2)")
  (net 15 TEST)
  (net 16 "Net-(Q1-Pad1)")
  (net 17 "Net-(R1-Pad2)")
  (net 18 "Net-(R2-Pad2)")
  (net 19 "Net-(R5-Pad2)")
  (net 20 "Net-(R6-Pad2)")
  (net 21 "Net-(U2-Pad6)")
  (net 22 "Net-(Y1-Pad3)")
  (net 23 "Net-(C7-Pad1)")
  (net 24 "Net-(C1-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +9V)
    (add_net GND)
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C10-Pad2)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(C8-Pad2)")
    (add_net "Net-(C9-Pad2)")
    (add_net "Net-(L2-Pad2)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(R6-Pad2)")
    (add_net "Net-(U2-Pad6)")
    (add_net "Net-(Y1-Pad3)")
    (add_net RST)
    (add_net TEST)
    (add_net VDD)
  )
  (net_class 50ohm ""
    (clearance 0.1524)
    (trace_width 0.7874)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C4-Pad2)")
    (add_net "Net-(C6-Pad2)")
  )
  (module DonB:C_0805_HandSoldering (layer F.Cu) (tedit 55C2E250)
    (at 126.873 86.36 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at -3.175 0 90) (layer F.SilkS))
    (fp_text value 1uF (at 0 0.127 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(C1-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:C_0805_HandSoldering (layer F.Cu) (tedit 559C2A21)
    (at 123.19 97.663 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 0 -1.778 90) (layer F.SilkS))
    (fp_text value 22pF (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:C_0805_HandSoldering (layer F.Cu) (tedit 559C2A34)
    (at 127.635 96.52 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at 0 -1.905 180) (layer F.SilkS))
    (fp_text value 12pF (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:C_0805_HandSoldering (layer F.Cu) (tedit 559C2A16)
    (at 118.999 97.663 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at 0 -1.778 90) (layer F.SilkS))
    (fp_text value 39pF (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C4-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:C_0805_HandSoldering (layer F.Cu) (tedit 55C2E115)
    (at 118.11 86.36 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at 0 1.778 270) (layer F.SilkS))
    (fp_text value 1uF (at 0 2.1 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:C_0805_HandSoldering (layer F.Cu) (tedit 559C2A0E)
    (at 114.935 97.663 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C6 (at 0 -1.778 90) (layer F.SilkS))
    (fp_text value 22pF (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C6-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:C_0805_HandSoldering (layer F.Cu) (tedit 559C2BF4)
    (at 145.415 91.44)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C7 (at -0.254 -1.651) (layer F.SilkS))
    (fp_text value 20pF (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(C7-Pad1)"))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:C_0805_HandSoldering (layer F.Cu) (tedit 559C2CA3)
    (at 145.415 99.314 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C8 (at -2.921 0 270) (layer F.SilkS))
    (fp_text value 1nF (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C8-Pad1)"))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C8-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:C_0805_HandSoldering (layer F.Cu) (tedit 559C2AD5)
    (at 156.845 97.79 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C9 (at 0 -1.524 90) (layer F.SilkS))
    (fp_text value 330nF (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C9-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:C_0805_HandSoldering (layer F.Cu) (tedit 559C2C2A)
    (at 154.94 88.265 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C10 (at 0 1.651 180) (layer F.SilkS))
    (fp_text value 470nF (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C10-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:C_0805_HandSoldering (layer F.Cu) (tedit 559C2D3A)
    (at 163.195 96.52 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C11 (at 3.302 -0.762 180) (layer F.SilkS))
    (fp_text value 1nF (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 12 RST))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:C_0805_HandSoldering (layer F.Cu) (tedit 559C2BED)
    (at 139.065 91.44 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C12 (at 0 1.651 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 13 VDD))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:C_0805_HandSoldering (layer F.Cu) (tedit 559C2C9A)
    (at 139.065 99.06 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C13 (at -2.921 -0.127 270) (layer F.SilkS))
    (fp_text value 100nF (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 13 VDD))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:C_0805_HandSoldering (layer F.Cu) (tedit 559C301E)
    (at 163.195 87.63 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C14 (at 3.556 0 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:R_0805_HandSoldering (layer F.Cu) (tedit 559C2A05)
    (at 121.92 93.345 180)
    (descr "Resistor, SMD, 0805, Hand soldering,")
    (tags "Resistor, SMD, 0805, Hand soldering,")
    (attr smd)
    (fp_text reference L1 (at 0 1.524 180) (layer F.SilkS))
    (fp_text value 68nH (at -0.08 1.524 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.30048 0 180) (size 1.50114 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad2)"))
    (pad 2 smd rect (at 1.30048 0 180) (size 1.50114 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C4-Pad2)"))
    (model smd/resistors/R0805/R0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:R_0805_HandSoldering (layer F.Cu) (tedit 559C2F11)
    (at 132.715 96.52)
    (descr "Resistor, SMD, 0805, Hand soldering,")
    (tags "Resistor, SMD, 0805, Hand soldering,")
    (attr smd)
    (fp_text reference L2 (at 0 1.905) (layer F.SilkS))
    (fp_text value 100nH (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.30048 0) (size 1.50114 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 1.30048 0) (size 1.50114 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(L2-Pad2)"))
    (model smd/resistors/R0805/R0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:R_0805_HandSoldering (layer F.Cu) (tedit 559C29F9)
    (at 116.205 93.345 180)
    (descr "Resistor, SMD, 0805, Hand soldering,")
    (tags "Resistor, SMD, 0805, Hand soldering,")
    (attr smd)
    (fp_text reference L3 (at 0 1.524 180) (layer F.SilkS))
    (fp_text value 68nH (at -0.08 1.524 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.30048 0 180) (size 1.50114 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C4-Pad2)"))
    (pad 2 smd rect (at 1.30048 0 180) (size 1.50114 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C6-Pad2)"))
    (model smd/resistors/R0805/R0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:TESTPIN (layer B.Cu) (tedit 544326E2)
    (at 137.16 86.36 180)
    (fp_text reference P1 (at 0 2 180) (layer B.SilkS) hide)
    (fp_text value 4-16V (at 0 -2 180) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.651 1.651) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 2 +9V))
  )
  (module DonB:TESTPIN (layer B.Cu) (tedit 544326E2)
    (at 142.24 86.36 180)
    (fp_text reference P2 (at 0 2 180) (layer B.SilkS) hide)
    (fp_text value GND (at 0 -2 180) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.651 1.651) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 1 GND))
  )
  (module DonB:TESTPIN (layer B.Cu) (tedit 559BFC2F)
    (at 158.75 85.09 90)
    (fp_text reference P4 (at 0 2 90) (layer B.SilkS) hide)
    (fp_text value 3.3V (at -3.175 0 90) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.651 1.651) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 6 +3V3))
  )
  (module DonB:TESTPIN (layer B.Cu) (tedit 559BFC34)
    (at 161.29 85.09 90)
    (fp_text reference P5 (at 0 2 90) (layer B.SilkS) hide)
    (fp_text value GND (at -3.175 0 90) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.651 1.651) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 1 GND))
  )
  (module DonB:TESTPIN (layer B.Cu) (tedit 559C10CB)
    (at 163.83 85.09 90)
    (fp_text reference P6 (at 0 2 90) (layer B.SilkS) hide)
    (fp_text value TEST (at -3.048 0 90) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.651 1.651) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 15 TEST))
  )
  (module DonB:TESTPIN (layer B.Cu) (tedit 559BFC3B)
    (at 166.37 85.09 90)
    (fp_text reference P7 (at 0 2 90) (layer B.SilkS) hide)
    (fp_text value RST (at -3.175 0 90) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.651 1.651) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 12 RST))
  )
  (module Housings_SOT-23_SOT-143_TSOT-6:SOT-23_Handsoldering (layer F.Cu) (tedit 559C2EB6)
    (at 132.715 91.44 270)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 0.889 3.683 360) (layer F.SilkS))
    (fp_text value BSS-223PW (at 0 3.81 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.50114 270) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at 0.95 1.50114 270) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 3 smd rect (at 0 -1.50114 270) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 13 VDD))
    (model Housings_SOT-23_SOT-143_TSOT-6.3dshapes/SOT-23_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:R_0805_HandSoldering (layer F.Cu) (tedit 559C2C13)
    (at 149.86 86.995 270)
    (descr "Resistor, SMD, 0805, Hand soldering,")
    (tags "Resistor, SMD, 0805, Hand soldering,")
    (attr smd)
    (fp_text reference R1 (at 0 -1.651 270) (layer F.SilkS))
    (fp_text value 4.7K (at -0.08 1.524 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.30048 0 270) (size 1.50114 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 13 VDD))
    (pad 2 smd rect (at 1.30048 0 270) (size 1.50114 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(R1-Pad2)"))
    (model smd/resistors/R0805/R0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:R_0805_HandSoldering (layer F.Cu) (tedit 559C2C10)
    (at 146.05 86.995 270)
    (descr "Resistor, SMD, 0805, Hand soldering,")
    (tags "Resistor, SMD, 0805, Hand soldering,")
    (attr smd)
    (fp_text reference R2 (at 0 -1.651 270) (layer F.SilkS))
    (fp_text value 4.7K (at -0.08 1.524 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.30048 0 270) (size 1.50114 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 13 VDD))
    (pad 2 smd rect (at 1.30048 0 270) (size 1.50114 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(R2-Pad2)"))
    (model smd/resistors/R0805/R0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:R_0805_HandSoldering (layer F.Cu) (tedit 559C2AD9)
    (at 153.67 97.79 90)
    (descr "Resistor, SMD, 0805, Hand soldering,")
    (tags "Resistor, SMD, 0805, Hand soldering,")
    (attr smd)
    (fp_text reference R3 (at 0 -1.524 90) (layer F.SilkS))
    (fp_text value 100K (at -0.08 1.524 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.30048 0 90) (size 1.50114 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C8-Pad1)"))
    (pad 2 smd rect (at 1.30048 0 90) (size 1.50114 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C9-Pad2)"))
    (model smd/resistors/R0805/R0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:R_0805_HandSoldering (layer F.Cu) (tedit 559C2CCC)
    (at 153.67 92.71 90)
    (descr "Resistor, SMD, 0805, Hand soldering,")
    (tags "Resistor, SMD, 0805, Hand soldering,")
    (attr smd)
    (fp_text reference R4 (at 0 -1.524 90) (layer F.SilkS))
    (fp_text value 680R (at -0.08 1.524 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.30048 0 90) (size 1.50114 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C9-Pad2)"))
    (pad 2 smd rect (at 1.30048 0 90) (size 1.50114 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C10-Pad2)"))
    (model smd/resistors/R0805/R0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:R_0805_HandSoldering (layer F.Cu) (tedit 559C2CD0)
    (at 156.845 92.71 270)
    (descr "Resistor, SMD, 0805, Hand soldering,")
    (tags "Resistor, SMD, 0805, Hand soldering,")
    (attr smd)
    (fp_text reference R5 (at 0 1.524 270) (layer F.SilkS))
    (fp_text value 470R (at -0.08 1.524 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.30048 0 270) (size 1.50114 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C10-Pad2)"))
    (pad 2 smd rect (at 1.30048 0 270) (size 1.50114 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(R5-Pad2)"))
    (model smd/resistors/R0805/R0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:R_0805_HandSoldering (layer B.Cu) (tedit 559C3175)
    (at 127 92.075 270)
    (descr "Resistor, SMD, 0805, Hand soldering,")
    (tags "Resistor, SMD, 0805, Hand soldering,")
    (attr smd)
    (fp_text reference R6 (at 0 1.778 270) (layer B.SilkS))
    (fp_text value 1.5K (at -0.08 -1.524 270) (layer B.SilkS) hide)
    (pad 1 smd rect (at -1.30048 0 270) (size 1.50114 1.19888) (layers B.Cu B.Paste B.Mask)
      (net 16 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at 1.30048 0 270) (size 1.50114 1.19888) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(R6-Pad2)"))
    (model smd/resistors/R0805/R0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:R_0805_HandSoldering (layer F.Cu) (tedit 559C2B39)
    (at 163.195 99.06 180)
    (descr "Resistor, SMD, 0805, Hand soldering,")
    (tags "Resistor, SMD, 0805, Hand soldering,")
    (attr smd)
    (fp_text reference R7 (at 3.175 0 180) (layer F.SilkS))
    (fp_text value 47K (at 0 -0.127 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.30048 0 180) (size 1.50114 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 12 RST))
    (pad 2 smd rect (at 1.30048 0 180) (size 1.50114 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (model smd/resistors/R0805/R0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOT-23_SOT-143_TSOT-6:SOT-23_Handsoldering (layer F.Cu) (tedit 55C2E10E)
    (at 123.19 86.36)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference U1 (at -2.159 -1.524 90) (layer F.SilkS))
    (fp_text value MCP1703 (at -2.54 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.50114) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.95 1.50114) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 3 smd rect (at 0 -1.50114) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(C1-Pad2)"))
    (model Housings_SOT-23_SOT-143_TSOT-6.3dshapes/SOT-23_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:MSOP-10_3x3mm_Pitch0.5mm (layer F.Cu) (tedit 559C2CE7)
    (at 139.065 95.25 180)
    (descr "10-Lead Plastic Micro Small Outline Package (MS) [MSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.5")
    (attr smd)
    (fp_text reference U2 (at 0 0 180) (layer F.SilkS))
    (fp_text value SI5351 (at 0 0.635 180) (layer F.Fab))
    (pad 1 smd rect (at -2.2 -1 180) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 13 VDD))
    (pad 2 smd rect (at -2.2 -0.5 180) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C8-Pad2)"))
    (pad 3 smd rect (at -2.2 0 180) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(C7-Pad1)"))
    (pad 4 smd rect (at -2.2 0.5 180) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(R2-Pad2)"))
    (pad 5 smd rect (at -2.2 1 180) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(R1-Pad2)"))
    (pad 6 smd rect (at 2.2 1 180) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(U2-Pad6)"))
    (pad 7 smd rect (at 2.2 0.5 180) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 13 VDD))
    (pad 8 smd rect (at 2.2 0 180) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at 2.2 -0.5 180) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(L2-Pad2)"))
    (pad 10 smd rect (at 2.2 -1 180) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(L2-Pad2)"))
    (model Housings_SSOP.3dshapes/MSOP-10_3x3mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SOIC-8-N (layer F.Cu) (tedit 559C2CEB)
    (at 163.195 92.075 270)
    (descr "Module Narrow CMS SOJ 8 pins large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference U3 (at 0 0 270) (layer F.SilkS))
    (fp_text value MSP430G2210 (at 0.889 -3.429 270) (layer F.Fab))
    (pad 8 smd rect (at -1.905 -3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 7 smd rect (at -0.635 -3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 15 TEST))
    (pad 6 smd rect (at 0.635 -3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 12 RST))
    (pad 5 smd rect (at 1.905 -3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(R6-Pad2)"))
    (pad 4 smd rect (at 1.905 3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(R5-Pad2)"))
    (pad 3 smd rect (at 0.635 3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(R2-Pad2)"))
    (pad 2 smd rect (at -0.635 3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(R1-Pad2)"))
    (pad 1 smd rect (at -1.905 3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (model SMD_Packages.3dshapes/SOIC-8-N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.38 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module DonB:SMA-142-0701-0801 (layer F.Cu) (tedit 559C2D93)
    (at 108.204 93.345 90)
    (fp_text reference P3 (at 0 4.445 90) (layer F.SilkS) hide)
    (fp_text value BNC (at 0 -10.795 90) (layer F.Fab))
    (pad 2 thru_hole circle (at -4.3815 3.429 90) (size 0.7112 0.7112) (drill 0.4572) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 smd rect (at -4.3815 2.54 90) (size 0.4572 0.889) (drill (offset 0 0.4445)) (layers *.Cu *.Paste *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 smd rect (at -4.3815 0 90) (size 2.413 5.08) (layers *.Cu *.Paste *.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0 0 90) (size 2.286 5.08) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C6-Pad2)"))
    (pad 2 smd rect (at 4.3815 0 90) (size 2.413 5.08) (layers *.Cu *.Paste *.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 4.3815 2.54 90) (size 0.4572 0.889) (drill (offset 0 0.4445)) (layers *.Cu *.Paste *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 4.3815 3.429 90) (size 0.7112 0.7112) (drill 0.4572) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
  )
  (module DonB:Diode_SOT23_Handsoldering (layer F.Cu) (tedit 55C2E3DB)
    (at 130.81 86.36)
    (descr "Diode, SOT23, Handsoldering, RevA, 03Aug2010,")
    (tags "Diode, SOT23, Handsoldering, RevA, 03Aug2010,")
    (attr smd)
    (fp_text reference D2 (at 1.524 -1.651) (layer F.SilkS))
    (fp_text value PMEG2010 (at 0 3.81) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1 1.50114) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 2 +9V))
    (pad 2 smd rect (at 1 1.50114) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 2 +9V))
    (pad 3 smd rect (at 0 -1.50114) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(C1-Pad2)"))
  )
  (module DonB:Diode_SOT23_Handsoldering (layer F.Cu) (tedit 559C2D68)
    (at 149.86 95.885 180)
    (descr "Diode, SOT23, Handsoldering, RevA, 03Aug2010,")
    (tags "Diode, SOT23, Handsoldering, RevA, 03Aug2010,")
    (attr smd)
    (fp_text reference D1 (at 1.143 3.302 180) (layer F.SilkS))
    (fp_text value SMV1213 (at 0 3.81 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1 1.50114 180) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1 1.50114 180) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 0 -1.50114 180) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C8-Pad1)"))
  )
  (module DonB:CRYSTAL-3.2x2.5 (layer F.Cu) (tedit 55B467DC)
    (at 145.415 95.25 90)
    (fp_text reference Y1 (at 0 -1.905 90) (layer F.SilkS))
    (fp_text value 27MHz (at 0 -3.81 90) (layer F.Fab))
    (pad 4 smd rect (at -1.15 -0.925 90) (size 1.9 1.2) (drill (offset -0.5 -0.075)) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 1.15 0.925 90) (size 1.9 1.2) (drill (offset 0.5 0.075)) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(Y1-Pad3)"))
    (pad 1 smd rect (at -1.15 0.925 90) (size 1.9 1.2) (drill (offset -0.5 0.075)) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C8-Pad2)"))
    (pad 2 smd rect (at 1.15 -0.925 90) (size 1.9 1.2) (drill (offset 0.5 -0.075)) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(C7-Pad1)"))
  )
  (module DonB:C_0805_HandSoldering (layer F.Cu) (tedit 55C2E3C7)
    (at 134.62 86.36 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C15 (at 2.413 -1.651 270) (layer F.SilkS))
    (fp_text value 10nF (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(C1-Pad2)"))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 +9V))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Don Bindner" (at 154.559 98.425) (layer B.SilkS))
  (gr_text "Morse Beacon" (at 126.619 98.425) (layer B.SilkS))
  (gr_line (start 105.283 100.33) (end 167.64 100.33) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 105.283 83.566) (end 167.64 83.566) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 167.64 83.566) (end 167.64 100.33) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 105.283 83.566) (end 105.283 100.33) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 167.259 99.949) (xy 105.664 99.949) (xy 105.664 83.947) (xy 167.259 83.947)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 167.259 99.949) (xy 105.664 99.949) (xy 105.664 83.947) (xy 167.259 83.947)
      )
    )
  )
)
